# C - Clutch

Tools
BCV BCP

This step will run the tool with the programmed Speed in forward direction until the Clutch has been released. When the tool has reported the release of the Clutch the step will finish with OK status.

A tightening program using the Clutch step cannot have any other step assigned.

This step is only valid for the Clutch tools BCV-RE and BCP-RE.

Parameter | Description
--- | ---
Speed Control | One Speed or Two Speed
Final Speed | Sets the final speed of the program [rpm]
Speed Ramp | Switch where speed ramp can be chosen [Hard, Soft]
Rehit | Rehit detection set to On or Off
Rehit angle | Sets the rehit angle [°]