# Activated Joint Id - 225

Set when a compatible task is configured and running with Joint Ids. When a program or batch is started where Joint Id is used, the signal is set with the corresponding configured Joint Id for the program that's is selected by an MES/Integrator/External system. The string indicates the currently active Joint Id and not the one in a result, please see “Joint Id Result - 31046” for Joint Ids tied to specific results. If automatic incrementation is used of the Joint Id within a batch the active Joint Id will be updated when next tightening in the batch is loaded. Please see Source Tightening Properties for further information about setup of Joint Id.

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | String | 8 | 800

## Devices

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE

- User Display: FALSE

- Soft Selector: FALSE

- Indicator Box: FALSE

- Automation Rules: FALSE

- Fieldbus: TRUE