# Tool Configuration

With the Tool Configuration it is possible to activate and configure various functions related to the tool. Each tool configuration can be mapped to a tool in Hardware Layout Configuration.

To view or edit a tool configuration menu:

1. Select a controller in the Plant structure workspace .

2. Click Configurations in the Menu bar.

   The workspace area displays the current accessory configurations.

3. Add a new configuration or double click on an existing configuration with the type being a tool configuration.

4. Make necessary configurations. The parameters are described in each section.

The tool configuration is divided into the following menus:

Menu | Description
--- | ---
Properties | Configuration name and description and a tool type filter.
General | General parameters for the tool.
Multiple transducer (only available for FlexSystem) | Multiple transducer functionality.
Tool LEDs (only available for Synchronized tightening) | See Tool Configuration - Tool LEDs.
Buzzer (only available for Synchronized tightening) | See Tool Configuration - Buzzer.

## Properties

The Tool configuration should be given a unique name. An optional description field is also available.

The accessory configuration list displays all configurations in an alphabetical order

To view or edit a tool configuration menu:

1. Select a controller in the Plant structure workspace .

2. Select the Configuration icon in the menu bar.

   The workspace area shows a list of all the current accessory configurations.

3. Double-click on the name of the selected Tool configuration.

   The workspace area shows the details of the current configuration and is divided into different menus, one for each topic.

4. Enter a configuration name and a description in the Properties menu.

5. Select a tool type from the Filter by tool type drop-down menu.

   As the number of tools grow, the number of menus grow as well. To increase the visual comfort in the workspace, it is possible to filter menus and only show what is relevant for one selected tool type. The filter is set in the Properties menu. If No tool is selected, all the possible tool configuration parameters are displayed.

## General

Use Start source to set how to start the tool.

Start source | Description
--- | ---
Trigger only | Press the tool trigger to start the tightening.
Trigger OR Push | Press the tool trigger or push the tool against the joint to start the tightening.
Trigger AND Push | Press the tool trigger and push the tool against the joint to start the tightening.
Push only | Push the tool against the joint to start the tightening.
Digital input | Using an external digital input signal to trigger the start of the tightening.
Safety trigger | Press the safety trigger (both Main Trigger and Extra Trigger) to start the tightening.

## Multiple transducers

Only available for QST and IxB tools.

Depending on the tool type and the number of transducers, it is possible to set how the torque and angle transducers are used in a tightening. The transducers can be configured to be controlling or monitoring.

Multiple transducers
Parameter | Description
--- | ---
Controlling torque transducer | Set the torque transducer to use for tightening. Available settings: Auto: For QST tools, Torque is used by default. For IxB tools, Torque 2 is used by default. If Torque 2 is not available for the IxB tool type, Torque is used. Torque Torque 2
Controlling angle transducer | Set the angle transducer to use for tightening. Available settings: Auto: For QST tools, Motor angle is used by default. Motor angle Angle Angle 2

Select Details to open a sub-menu with more settings.

Monitor and reporting torque
Parameter | Description
--- | ---
Report monitoring torque values | If set, a Final Torque value will be reported from both the controlling and the monitoring transducer, including evaluation of the status for both (OK/High/Low).
Redundancy error reporting torque | Redundancy error is reported if the Final Torque measured on the controlling transducer differ from the value measured on the monitoring transducer.
Lock the tool on redundancy error | Lock the tool if a redundancy error is detected.

Torque transducer misc settings
Parameter | Description
--- | ---
Require dual torque | If set, the connected tool must have dual torque transducers (that are not disabled) to be able to run a tightening.
Monitoring torque in trace | If set, the values from the monitoring torque transducer are included in the trace.

Dual torque restrictions
Parameter | Description
--- | ---
Enable double torque restriction | If set, the double torque transducer restriction is active.
Maximum torque difference | The limit for the double torque difference restriction.

Monitor and reporting angle
Parameter | Description
--- | ---
Report monitoring angle values | If set, a Final Angle value will be reported from both the controlling and the monitoring transducer, including evaluation of the status for both (OK/High/Low).
Redundancy error reporting angle | Redundancy error is reported if the Final Angle measured on the controlling transducer differ from the value measured on the monitoring transducer.
Lock the tool on redundancy error | Lock the tool if a redundancy error is detected.

Angle transducer misc settings
Parameter | Description
--- | ---
Require dual angle | If set, the connected tool must have dual angle transducers (that are not disabled) to be able to run a tightening.
Monitoring angle in trace | If set, the values from the monitoring angle transducer is included in the trace.

Dual angle restrictions
Parameter | Description
--- | ---
Enable double angle restriction | If set, the double angle transducer restriction is active.
Maximum angle difference | The limit for the double angle difference restriction.