# Triggering Manual Mode

Manual Mode can be activated by a switch or an external system. For example (indicated below), a key switch on an operator panel can be configured to activate manual mode.

1. Go to the Configurations menu and choose Operator panel .

2. In the configuration window, go to the position [A,B,C,D,E,F,G,I] to configure and in the list, choose One way key switch.

3. Select on the Turn signal list. In the list, choose Manual mode.

4. Close the window.

If the user needs to be notified that Manual mode has been entered or left, then events 4070 and 4071 have to be configured, respectively. This is done in Settings - Events.

Relevant Information

- Configuring Manual Mode
- Events Menu
- Pushing Configurations to a Controller