# Final Angle Status - 31006

This signal shows the status of the final angle, which can be:

- OK - if the measured angle is within the limits configured in the tightening program.

- HIGH - if the measured angle is more than the high limit configured in the tightening program.

- LOW - if the measured angle is less than the low limit configured in the tightening program.

The value of the Final Angle Status signal shows differently, depending on the configuration of the fieldbus signal.
If the user selects the signal converter, the signal shows one of the following values:

- O - Final Angle Status OK.

- H - Final Angle Status High.

- L - Final Angle Status Low.

If there is no filter applied, the signal shows one of the following values:

- 1 - Final Angle Status OK.

- 2 - Final Angle Status High.

- 3 - Final Angle Status Low.

Name in SoftPLC: FINAL_ANGLE_STATUS

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Integer | 2 | 8
StatusAsChar | State | Integer | 2 | 8

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE