# Data Drop Active - 199

This signal will be set high whenever DATADROP function is active. When DATADROP input signal is set and worktask supporting DATADROP is selected.

Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | ---
State | Boolean | 1 | 1

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE