# Tool Configuration - General Configuration

Inactivity timeout | Description
--- | ---
On | Only valid for battery tools. In order to save battery time there is an option to automatically turn off the tool after a certain time of inactivity. Enter a value between 1-1440 minutes.
Off | The tool will not be turned off due to inactivity.

Front LED | Description
--- | ---
Front LED enabled | Wireless tools: Off - Tool Front LED will always be off. On - Front LED is lit when the tool trigger is pressed, plus time set in Front LED duration starting at trigger release. Cable tools: The front LED is lit for 10 seconds after the tool trigger has been pressed.
Front LED duration | Wireless tools: Front LED duration in seconds, starting when the tool trigger is released.

Use Start source to set how to start the tool.

Start source | Description
--- | ---
Trigger only | Press the tool trigger to start the tightening.
Trigger OR Push | Press the tool trigger or push the tool against the joint to start the tightening.
Trigger AND Push | Press the tool trigger and push the tool against the joint to start the tightening.
Push only | Push the tool against the joint to start the tightening.
Digital input | Using an external digital input signal to trigger the start of the tightening.
Safety trigger | Applicable only on tools that have two triggers. The two triggers must be pressed simultaneously to start a tightening or loosening. Both triggers must be released between consecutive tightenings.

Use Trace start to set how to start the tightening trace.

Trace start | Description
--- | ---
Off | No data tracing.
Trigger pressed | Data tracing of the tightening process starts as soon as the trigger is pressed.
Rundown complete | Data tracing of the tightening process starts when the Rundown complete is detected.

The Start request switch defines the action when communication between tool and controller is lost.

Start request enables the requirement of having a connection between the tool and the controller, for all battery tools. This to make sure that the tool is always up to date with tightening program or batch settings, and with other settings on the controller, when performing tightenings.

When Start request is set to On, the tool becomes locked if the controller connection is lost. This means that if the tool loses connection in the middle of a tightening or a batch sequence, the tool will finish the ongoing tightening and then stop. The tool will be locked until the connection is re-established.

Start request | Description
--- | ---
On | The current Tightening program is finished and subsequent tightenings are stopped when the connection is lost between the controller and the tool.
Off | Current Tightening program or Batch can be finished even if the connection is lost between controller and tool.

The TAG number is the RFID TAG which is used to identify the end-fitting tool in the STwrench. The following options are available:

TAG check | Description
--- | ---
On | Check the TAG number of the End-fitting tool (socket). The TAG number must be identical to the number in the Tightening program configuration.
Off | No TAG checking is done.

TAG selection | Description
--- | ---
On | Use the TAG number of the End-fitting tool (socket) to select a batch in a batch sequence. The TAG number must be written into the identifier number field in the Sequence configuration menu in the batch sequence section .
Off | The TAG value is not used to select a batch.

Lock tool on memory full gives the tool the possibility to perform tightenings even when the tool memory is full. This means that the tightenings performed when the tool memory is full will never be reported to the controller.

Lock tool on memory full | Description
--- | ---
On | The tool will be locked from further tightening operations when the tool memory is full. In order to resume tightening operations the tool has to reestablish connection to the controller and send the tightening results that have been stored in the tool memory.
Off | The tool will continue to perform tightenings even when the tool memory is full.