# Bolt or Channel Area Overview

In the bolt or channel configuration area, it is possible to configure the acyclic data items of the following types for a bolt or a channel:

- MultiStage tightening

- Program monitor

- Program restriction

- Step monitor

- Step restriction

Bolt or channel area properties
Parameter name | Description
--- | ---
Type | Value type of each item. Example: MultiStage tightening, Program monitor, Program restriction, Step monitor or Step restriction.
Offset | Item position in the acyclic data frame and is defined in bytes.
Size | Size in bytes. It is possible to configure this manually if the datatype is a string. If the datatype is not a string, the values are set automatically based on the data type.
Data type | Data type values. Example: String, Int8, Int16 and so on.
Name | Item name. Non editable.
Identifier | Sets the ID of the bolt or channel selected.

Relevant Information

- Acyclic Result Items

In this Section

- Adding Acyclic Result Configuration in the Bolt or Channel Area
- Creating Copies in the Bolt or Channel Area
- Deleting Acyclic Result Configuration from Bolt or Channel Area