# Adding Acyclic Result Configuration in Common Area

1. Select Add in the Common area.

   The Create acyclic result configuration window opens.

2. Select a parameter from the Multiple tightening, Result notification or Batch sequence drop-down menu.

3. Select the Output Data Type, enter the offset value and enter the size if the Output Data Type selected was a string.

4. Select Add and then select Close.