# General Virtual Station

Adding a General Virtual Station

1. In the Plant structure workspace , select a controller.

2. In the tab menu bar in the workspace area, select the Configurations icon .

   The workspace area displays a list of configurations.

3. Double-click on a configuration row that has General Virtual Station in the Type column.

   Alternatively, select Add to create a new General Virtual Station configuration .

Properties
Parameter | Description
--- | ---
Name | Optional name for the configuration
Description | Optional configuration description

When using Synchronized tightening or a Flex controller the following parameter is also visible in the General Virtual Station configuration.

Fixtured Stations

Auto Enable can use one of the following settings, the default setting is Never.

Setting | Description
--- | ---
Never | Input Enable Operation must be set high to be able to run a tightening.
Always | It is always possible to run tightenings regardless of the status of input Enable Operation.

To apply the General Virtual Station configuration, assign it to a Virtual Station in the Virtual Station section.

Only unassigned General Virtual Station configurations can be deleted.

Relevant Information

- Assigning a General Virtual Station Configuration
- Global Configurations Library - Creating a Global Configuration From An Existing
- Pushing Configurations to a Controller
- Working with the Configurations Tab