# Adding a New Acyclic Data Configuration

1. Select a controller in the Plant structure .

2. Go to Fieldbus and SoftPLC tab .

3. Select the Acyclic sub-tab.

4. Select Add and select New in the Create new acyclic data configuration window.

5. Enter the acyclic data configuration name and select Add.

   The Properties sub-tab for the newly created configuration opens.

   A new acyclic data configuration is added in the lowest possible position and the list is updated.

In this Section

- Acyclic Data Configuration Menu
- Configure Acyclic Data