# Ti - Time

Tools
ES STR SL ST SR QST STB IXB

Measures the elapsed time during the monitor and checks that it is between the time limits. The time measurement starts at the start of the monitor and, if the Trigger Torque is specified, at the point where the torque passes Trigger Torque for the first time during the monitor.

Parameter | Description
--- | ---
Trigger Torque | Must be >= 0 and < Tool max torque.
Low Limit | Must be >= 0
High Limit | Must be > 0 Must be > Low limit