# Event Codes

Different types of events are used to notify the user of certain state changes or occurrences in the system. Each event requires a different action.

Some of the procedures described can only be performed by Atlas Copco Service personnel.

For more information about a specific event code, use the below filters or enter the event code search criteria in the search box.

Event Code
Event Type
Event Name
Description
Procedure
Log / Display / Ack / Conf
Available for
Group
Search

Event Code | Event Type | Event Name | Description | Procedure | Log / Display / Ack / Conf | Available for | Group
--- | --- | --- | --- | --- | --- | --- | ---
none | item | none | none | none | column | list | list
1000 | Info | Controller Started | The controller is started. |  | Log Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC Power Focus HC ToolsControl | Controller and Tool
1001 | Warning | Controller Serial Number Updated | Generated at start-up if IT-board box serial number (controller serial number) differs from AUX-board box serial number. AUX-board is considered to be non-replaceable in field. The controller will reboot when the serial number is updated. | Replace IT-board or box. | Log Display Ack Conf | Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC | Controller and Tool
1010 | Info | Tool Connected | A tool is connected. |  | Log Display Conf | Flex Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC Power Focus HC ToolsControl | Controller and Tool
1011 | Info | Tool Disconnected | A tool is disconnected. |  | Log Display Conf | Flex Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC Power Focus HC ToolsControl | Controller and Tool
1012 | Info | Tool Rejected Controller Connection | This event can occur if the tool is into a skip-zone. | Verify if another controller is connected to the tool. Make sure that the tool settings are correctly set up. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Controller and Tool
2000 | Warning | Battery Low |  | Replace battery. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl XB | Tool
2001 | Warning | Battery Empty |  | Replace battery. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl XB | Tool
2002 | Warning | Tool Battery Health Low | Tool battery health problem is detected. Valid for SRB, TBP and IxB tools only. | Replace battery. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2004 | Warning | Tool is not of the preferred type | Tool has been replaced by a tool with a different Tool Max Torque. | Change tool. | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2006 | Warning | Tool Backup Battery Health low | The backup battery in the tool has too poor performance. | The backup battery should be replaced. | Log Display Ack Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2007 | Warning | Tool Backup Battery Missing or Broken | Tool backup battery is missing or broken. Valid for SRB and TBP tools only. | Insert battery. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2008 | Warning | Tool Backup Battery Error | Tool backup battery error detected. Valid for SRB and TBP tools only. | Replace battery. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2009 | Warning | Backup Battery Voltage Low | The controller's backup battery is almost empty. | Replace battery. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2010 | Error | Tool Software Version Mismatch | Tool and controller software versions not compatible. | Service tool - update tool software. | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tool
2012 | Warning | Tool Communication Disturbance | Communication between tool and controller interrupted. | Relocate antenna placement. | Conf | Flex Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC Power Focus HC ToolsControl | Tool
2013 | Warning | Illegal Ring Position | Tool direction switch in faulty position. | If occurring frequently - service the tool. | Log Display Conf | Flex Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2014 | Warning | Tool Overheated | Tool overheated. Valid for SRB, TBP and IxB tools only. | Allow tool to cool down. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl XB | Tool
2015 | Error | Tool Temperature Sensor Error | SRB, TBP and IxB tools only. | Service the tool. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tool
2016 | Warning | Tool Pulse Unit Overheated | Pulse unit overheated. Tool is not locked, but the warning is displayed whenever the tool is started as long as the pulse unit temperature is over threshold. Valid for SRB, TBP and IxB tools only. | Allow tool to cool down. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2019 | Warning | Tool Could not Start Motor | Tool motor failure. Valid for SRB, TBP and IxB tools only. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2020 | Warning | Tool Requires Motor Tuning | Tool requires motor tuning. | Perform a motor tuning. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl XB | Tool
2021 | Warning | Motor Tuning Failed | Motor tuning failed. | Complete motor tuning or service the tool. | Log | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tool
2022 | Info | Motor Tuning Completed | Motor tuning completed. |  | Log Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tool
2023 | Warning | The Tool Requires Open End Tuning | The tool requires open end tuning. | Perform open end tuning. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2024 | Warning | Open End Tuning Failed | Open end tuning failed. | Try to perform open end tuning one more time. If it fails again, service the tool. | Log Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2025 | Info | Open End Tuning Successful | Open end tuning successful. |  | Log Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2026 | Warning | Open End Position Failed | Open end position failed. | Press the tool trigger again and wait for the positioning to be completed. If it fails again, service the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2027 | Warning | Usage Limited Due To High Tool Temperature | Temperature limit value has been reached. Tightening has been inhibited to reduce risk for tool shutting down due to overheating. | Wait until tool temperature has been reduced. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl XB | Tool
2030 | Error | Tool Memory Failure: Change Tool | Tool memory corrupt. | Service the tool. | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tool
2031 | Error | Tool Accessory Memory Corrupt | Tool accessory memory corrupt. | Service the tool accessory. | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tool
2040 | Error | System Check Failure |  |  | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl XB | Tool
2041 | Error | Torque Transducer Error | Will be generated either on calibration error or if tool reports transducer error. | Service the tool. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl XB | Tool
2042 | Error | Angle Transducer Error |  | Service the tool. | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tool
2043 | Error | Tool Ground Fault Error |  | Service the tool. | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tool
2044 | Info | Tool Service Interval Expired | Indicates that servicing of the tool is needed. Triggered when the number of set tightenings has been exceeded. | Perform service of tool. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tool
2045 | Warning | Tool Calibration Data Invalid | If validation of calibration data fails. | Service the tool. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl XB | Tool
2046 | Info | Tool: Next Calibration Date Has Passed | Indicates that calibration of tool is needed. Triggered when calibration alarm is enabled in settings and the current time is greater than next calibration date. | Service the tool. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tool
2048 | Info | Tool Calibration Value Updated By QA Device | Tool calibration was updated when a calibration with a QA device was performed. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2050 | Error | Tool Parameter File Not Supported | Required tool parameters are missing. | Update tool parameters. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tool
2060 | Info | Unexpected Trigger Behavior | Used to prevent start of tool if accessory is connected. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tool
2071 | Error | Tool Memory Corrupt | Tool descriptor is corrupt. | Service the tool. | Log Display Conf | Flex Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tool
2072 | Info | Unknown Device Connected |  |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tool
2073 | Warning | Tool Trigger Supervision Failure | HW channel failure. Mismatch between hardware and software of tool trigger. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2074 | Warning | Tool Indicator Board Failure | Tool indicator board failure. | Service the tool. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tool
2075 | Warning | Tool Fan Voltage Failure | Tool fan voltage failure. | Service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tool
2076 | Warning | Tool Accessory Bus Voltage Failure | Tool accessory bus voltage failure. | Service the tool. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tool
2077 | Warning | Tool Trigger Sensor Error | Tool trigger sensor error. | Service the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tool
2078 | Info | Tool Tightening Program Updated | Tool locked due to tightening program update. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2079 | Error | Tool Cable Not Supported | Tool cable is corrupt. The chip in the cable is not responding or is damaged. | Switch cable. | Log Display Conf | Flex Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tool
2080 | Error | Tool Battery Failure | DC voltage too high or too low. Battery failure. | Contact the Atlas Copco service representative and send back battery to Atlas Copco (do not reuse it!). | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl XB | Tool
2081 | Error | Tool Current Limit Reached | The current limit value has been reached and the drive is disabled. | Service the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2082 | Error | Tool Current Measurement Error | Current measurement error. Current cannot be measured with a reliable result. | Service the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl XB | Tool
2083 | Error | Tool Internal Error | Various internal hardware errors. Valid for STB and IxB tools only. | Service the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl XB | Tool
2084 | Error | Tool Internal Software Error | Various internal software errors. Valid for STB and IxB tools only. | Service the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl XB | Tool
2085 | Error | Tool RBU Error | An RBU error was detected by the tool software. | Check that the RBU is correctly installed. If error is still present then service the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2086 | Error | Tool Stall | Tool motor is stalling. | Service the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl XB | Tool
2087 | Warning | Tool Motor Current High | Tool motor current limit value is exceeded, and the tool is locked. Tool will enter failsafe mode. Valid for SRB, TBP and IxB tools only. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl XB | Tool
2088 | Warning | Tool Battery Current High | Tool battery current is too high. Valid for SRB, TBP and IxB tools only. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl XB | Tool
2089 | Warning | Tool Drive Voltage Low | Tool drive voltage is below the monitored lower voltage limit value. Valid for SRB, TBP and IxB tools only. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2090 | Warning | Tool Drive Voltage High | Tool drive voltage is above monitored higher voltage limit value. Valid for SRB, TBP and IxB tools only. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2091 | Warning | Tool Main Board Error | Tool main board internal error. Valid for SRB, TBP and IxB tools only. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl XB | Tool
2092 | Warning | Tool Power Module Error | Tool power module internal error. Valid for SRB, TBP and IxB tools only. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2093 | Warning | Pulse Unit Oil Level Low | The oil level of the connected pulse tool is low. | Service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2094 | Warning | Pulse Unit Oil Level Empty | The oil level of the connected pulse tool is below required operational level. | Service the tool. | Log Display Ack Conf | Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2095 | Warning | Tool Battery Communication Lost | Tool lost communication with battery. Valid for SRB, TBP and IxB tools only. | Make sure battery is snugged correctly. Otherwise change battery. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2096 | Error | Tool Battery Software Version Mismatch | Tool battery software incompatible with tool software. Valid for SRB, TBP and IxB tools only. | Update software. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2100 | Info | STwrench smartHEAD Removed | STwrench smartHEAD has been removed. | Reconnect smartHEAD and restart the wrench. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2101 | Warning | Wrench Tightening When Locked | A wrench tightening was performed when the tool status was locked in the controller. | Wait until the tool status in controller is unlocked. | Log Display Conf | Power Focus 6000 Power Focus 8 ToolsControl | Tool
2120 | Warning | Unable To Start: Tool Has No Active Torque Transducer |  |  | Log Display | Flex | Tool
2121 | Warning | Transducers Are Disabled For Connected Tool |  |  | Log Display | Flex | Tool
2122 | Warning | Unable To Start: Tool Is Missing Required Torque Transducer |  | Change to a tool with multiple torque transducers or update the setting "Require dual torque" in Tool Configuration. | Log Display | Flex IxB | Tool
2123 | Warning | Unable To Start: Tool Is Missing Required Angle Transducer |  | Change to a tool with multiple torque transducers or update the setting "Require dual torque" in Tool Configuration. | Log Display | Flex | Tool
2125 | Error | Torque Transducer Error On Transducer 2 | There is an error on torque transducer 2 of a tool with multiple transducers. | Service the tool. | Log Display | Flex | Tool
2127 | Error | Tool Torque Transducer Calibration Error | There is an error on the torque transducer. | Service the tool. | Log Display | Flex Synchronized tightening | Tool
2129 | Error | Tool Torque Transducer: Shunt Test Failed | There is an error on the torque transducer. | Service the tool. | Log Display | Flex Synchronized tightening XB | Tool
2131 | Error | Tool Torque Transducer: Zero Offset Compensation Failed | There is an error on the torque transducer. | Ensure the tightening is started with zero torque on the tool. Service the tool. | Log Display | Flex Synchronized tightening | Tool
2133 | Error | Tool Torque Transducer Hardware Error | There is an error on the torque transducer. | Service the tool. | Log Display | Flex Synchronized tightening | Tool
2135 | Error | Tool Torque Transducer Error: Overflow In A/D Converter | There is an error on the torque transducer. | Service the tool. | Log Display | Flex Synchronized tightening | Tool
2136 | Error | Tool Torque Transducer Calibration Error On Transducer 2 | There is an error on torque transducer 2 of a tool with multiple transducers. | Service the tool. | Log Display | Flex | Tool
2137 | Error | Tool Torque Transducer Error: Shunt Test Failed On Transducer 2 | There is an error on torque transducer 2 of a tool with multiple transducers. | Service the tool. | Log Display | Flex | Tool
2138 | Error | Tool Torque Transducer Error: Zero Offset Compensation Failed On Transducer 2 | There is an error on torque transducer 2 of a tool with multiple transducers. | Ensure the tightening is started with zero torque on the tool. Service the tool. | Log Display | Flex | Tool
2139 | Error | Tool Torque Transducer Hardware Error On Transducer 2 | There is an error on torque transducer 2 of a tool with multiple transducers. | Service the tool. | Log Display | Flex | Tool
2140 | Error | Tool Torque Transducer Error: Overflow In A/D Converter On Transducer 2 | There is an error on torque transducer 2 of a tool with multiple transducers. | Service the tool. | Log Display | Flex | Tool
2141 | Error | Tool Angle Transducer Error On Transducer 2 | Will be generated if tool reports transducer error from angle transducer 2. | Service the tool. | Log Display Conf | Flex Power Focus 6000 ToolsControl Power Focus 8 Synchronized tightening Power Focus XC | Tool
2142 | Error | Torque transducer redundancy error | There is an error on torque transducer 2 of a tool with multiple transducers. | Reset redundancy error | Log Display | Power Focus 6000 ToolsControl | Tool
2143 | Error | Angle transducer redundancy error | There is an error on torque transducer 2 of a tool with multiple transducers. | Reset redundancy error | Log Display | Power Focus 6000 ToolsControl | Tool
2144 | Warning | Tool Angle Transducer 2 Needs Calibration | Angle Transducer 2 needs calibration. | Tool requires motor tuning. | Log Conf Display | Flex Power Focus 6000 ToolsControl Power Focus 8 Synchronized tightening Power Focus XC | Tool
2145 | Warning | Tool Angle Transducer 3 Needs Calibration | Angle Transducer 3 needs calibration. | Tool requires motor tuning. | Log Conf Display | Flex Power Focus 6000 ToolsControl Power Focus 8 Synchronized tightening Power Focus XC | Tool
2146 | Error | Tool Angle Transducer Error on Transducer 3 | Will be generated if tool reports transducer error from angle transducer 3. | Service the tool. | Log Conf Display | Flex Power Focus 6000 ToolsControl Power Focus 8 Synchronized tightening Power Focus XC | Tool
2162 | Error | Torque transducer error: Torque value too low | Detected value below limits on torque transducer. | Restart the tool. If the problem persists, service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 Flex Synchronized tightening ToolsControl | Tool
2163 | Error | Torque transducer error: Torque value too high | Detected value above limits on torque transducer. | Restart the tool. If the problem persists, service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 Flex Synchronized tightening ToolsControl | Tool
2164 | Error | Torque transducer 2 error: Torque value too low | Detected value below limits on torque transducer 2. | Restart the tool. If the problem persists, service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 Flex Synchronized tightening ToolsControl | Tool
2165 | Error | Torque transducer 2 error: Torque value too high | Detected value above limits on torque transducer 2. | Restart the tool. If the problem persists, service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 Flex Synchronized tightening ToolsControl | Tool
2166 | Error | Tool restarted after an unexpected internal software error. | Tool was restarted after an unexpected internal software error. | Service the tool if problem persists. | Log Display Conf | Power Focus 6000 Power Focus 8 Flex Synchronized tightening ToolsControl | Tool
2167 | Error | Tool internal communication error on transducer module. | Tool internal communication error on transducer module. | Restart the tool. If the problem persists, service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 Flex Synchronized tightening ToolsControl | Tool
2168 | Error | Tool internal communication error on transducer module 2. | Tool internal communication error on transducer module 2. | Restart the tool. If the problem persists, service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 Flex Synchronized tightening ToolsControl | Tool
2169 | Error | Tool internal communication error with transducer module | Tool internal communication error with transducer module. | Restart the tool. If the problem persists, service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 Flex Synchronized tightening ToolsControl | Tool
2170 | Error | Tool transducer module error - Voltage out of range (Vdda on board 2) | Vdda votage is out of range on board 2 of tool transducer module. | Restart the tool. If the problem persists, service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 Flex Synchronized tightening ToolsControl | Tool
2171 | Error | Tool transducer module 2 error - Voltage out of range (Torque) | Torque supply voltage is out of range on torque transducer module 2. | Restart the tool. If the problem persists, service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 Flex Synchronized tightening ToolsControl | Tool
2174 | Error | Tool transducer module error - Voltage out of range (Vdda on board 1) | Vdda votage is out of range on board 1 of tool transducer module. | Restart the tool. If the problem persists, service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 Flex Synchronized tightening ToolsControl | Tool
2175 | Error | Tool transducer module error - CPU temperature high on board 1 | CPU temperature is high on board 1 of torque transducer module. | Wait until tool temperature has been reduced. If the problem persists, service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 Flex Synchronized tightening ToolsControl | Tool
2176 | Error | Tool transducer module error - CPU temperature high on board 2 | CPU temperature is high on board 2 of torque transducer module. | Wait until tool temperature has been reduced. If the problem persists, service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 Flex Synchronized tightening ToolsControl | Tool
2177 | Error | Tool torque transducer production calibration missing. | Production calibration parameters are missing on torque transducer module. | Restart the tool. If the problem persists, service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 Flex Synchronized tightening ToolsControl | Tool
2178 | Error | Tool transducer module error - Voltage out of range (Torque) | Torque supply voltage is out of range on torque transducer module. | Restart the tool. If the problem persists, service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 Flex Synchronized tightening ToolsControl | Tool
2179 | Error | Tool transducer module 2 error - Voltage out of range (Vdda on board 1) | Vdda votage is out of range on board 1 of tool transducer module 2. | Restart the tool. If the problem persists, service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 Flex Synchronized tightening ToolsControl | Tool
2180 | Error | Tool transducer module 2 error - CPU temperature high on board 1 | CPU temperature is high on board 1 of torque transducer module 2. | Wait until tool temperature has been reduced. If the problem persists, service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 Flex Synchronized tightening ToolsControl | Tool
2181 | Error | Tool transducer module 2 error - CPU temperature high on board 2 | CPU temperature is high on board 2 of torque transducer module 2. | Wait until tool temperature has been reduced. If the problem persists, service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 Flex Synchronized tightening ToolsControl | Tool
2182 | Error | Tool torque transducer 2 production calibration missing. | Production calibration parameters are missing on torque transducer module 2. | Restart the tool. If the problem persists, service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 Flex Synchronized tightening ToolsControl | Tool
2183 | Error | Tool transducer module 2 error - Voltage out of range (Vdda on board 2) | Vdda votage is out of range on board 2 of tool transducer module 2 | Restart the tool. If the problem persists, service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 Flex Synchronized tightening ToolsControl | Tool
2202 | Error | Tool HMI overcurrent occurred | Tool HMI overcurrent was detected. | Service the tool. Replace tool HMI. | Log Display Ack Conf | IxB | Tool
2203 | Error | Tool front light overcurrent occurred | Tool front light overcurrent was detected | Service the tool. Replace tool front light. | Log Display Ack Conf | IxB | Tool
2204 | Error | Accessory bus overcurrent occurred | Accessory bus overcurrent was detected. | Service the tool. Replace accessory bus. | Log Display Ack Conf | IxB | Tool
2207 | Error | Vibrator overcurrent occurred | Vibrator overcurrent was detected. | Service the tool. Replace the vibrator. | Log Display Ack Conf | IxB | Tool
2208 | Warning | System CPU temperature high | System CPU temperature high. | Wait until tool temperature has been reduced. | Log Display Conf | IxB XB | Tool
2209 | Error | System CPU temperature critical | System CPU temperature critical. | Wait until tool temperature has been reduced. | Log Display Conf | IxB XB | Tool
2210 | Error | Unsupported power source: tightening not permitted | Battery with too low voltage attached to the tool. | Attach battery with higher voltage to the tool. | Log Display Ack Conf | IxB | Tool
2217 | Info | Running on backup battery | Running on backup battery. |  | Log | IxB | Tool
2218 | Info | Battery connected | Battery connected or controller/tool started. |  | Log | IxB | Tool
2219 | Info | Power source: unknown | Unknown power source connected or controller/tool started with unknown power source. |  | Log | IxB | Tool
2220 | Error | Tool fan failure | Applies to IPB-P. | Service the tool. | Log Display Ack | IxB | Tool
2221 | Warning | Battery overheated | Battery temperature is too high. | Change battery and let overheated battery cool down. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 ToolsControl | Tool
2222 | Warning | Usage limited due to high battery temperature | Battery temperature is too high. | Change battery and let overheated battery cool down. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 ToolsControl | Tool
2223 | Error | Front LED is not available | When the tool boots up, if the front LED is not detected, this event will be triggered. | Fix the front light or the front light cable connection. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 | Controller and Tool
2224 | Error | Front LED color is not available | When the tool boots up, if the front LED color is not detected, this event will be triggered. | Fix the front light color or the front light cable connection | Log Display Conf | IxB Power Focus 6000 Power Focus 8 | Controller and Tool
2225 | Error | RHMI buttons are not available | When the tool boots up, if the RHMI buttons are not detected, an event will be triggered. | Fix the RHMI buttons. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 | Controller and Tool
2226 | Error | LED ring is not available | When the tool boots up, if the LED ring is not detected, an event will be triggered. | Fix the back ring lights or the back ring light connection. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 | Controller and Tool
2227 | Error | Fan is not available | When the tool boots up, if the fan is not detected, an event will be triggered. | Fix the fan. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 | Controller and Tool
2228 | Error | RRE board is not available | When the tool boots up, if the tool board interface is not detected, an event will be triggered. | Fix the tool board interface. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 | Controller and Tool
2229 | Warning | Tool Backup battery empty | Tool backup battery is empty. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2230 | Info | Tool Backup battery fully charged | Tool backup battery is fully charged. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2231 | Warning | Tool Backup Battery Missing | Tool backup battery is missing. | Insert battery. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2232 | Warning | Tool Backup Battery Broken | Tool backup battery is broken. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tool
2300 | Error | Tool main board error - Voltage out of range (Torque) |  | Restart the tool. If the error persist, service the tool an look for lose connections in the cable connectors. Inspect any possible damage in the cables. | Log Display Ack | IxB | Tool
2301 | Error | Tool main board error - Voltage out of range (Analog) |  | Restart the tool. If the error persist, service the tool an look for lose connections in the cable connectors. Inspect any possible damage in the cables. | Log Display Ack | IxB | Tool
2302 | Error | Tool main board error - Voltage out of range (MCU Vdd) |  | Restart the tool. If the error persist, service the tool an look for lose connections in the cable connectors. Inspect any possible damage in the cables. | Log Display Ack | IxB | Tool
2303 | Error | Tool main board error - Voltage out of range (Step up) |  | Restart the tool. If the error persist, service the tool an look for lose connections in the cable connectors. Inspect any possible damage in the cables. | Log Display Ack | IxB | Tool
2304 | Error | Tool main board error - Voltage out of range (UPS) |  | Restart the tool. If the error persist, service the tool an look for lose connections in the cable connectors. Inspect any possible damage in the cables. | Log Display Ack | IxB | Tool
2305 | Error | Tool main board error - Voltage out of range (Tool power) |  | Restart the tool. If the error persist, service the tool an look for lose connections in the cable connectors. Inspect any possible damage in the cables. | Log Display Ack | IxB XB | Tool
2306 | Error | Tool main board error - Voltage out of range (Vdd) |  | Restart the tool. If the error persist, service the tool an look for lose connections in the cable connectors. Inspect any possible damage in the cables. | Log Display Ack | IxB XB | Tool
2307 | Error | Tool main board error - Hardware failure (IMU) |  | Service the tool. | Log Display Ack | IxB | Tool
2331 | Error | Tool power module error - Voltage low (Reference) |  | Service the tool. | Log Display Ack | IxB | Tool
2332 | Error | Tool power module error - Voltage high (Reference) |  | Service the tool. | Log Display Ack | IxB | Tool
2333 | Error | Tool power module error - Voltage low (UPS) |  | Service the tool. | Log Display Ack | IxB | Tool
2334 | Error | Tool power module error - Voltage high (UPS) |  | Service the tool. | Log Display Ack | IxB | Tool
2335 | Error | Tool power module error - Voltage low (Backup domain) |  | Service the tool. | Log Display Ack | IxB | Tool
2336 | Error | Tool power module error - Voltage high (Backup domain) |  | Service the tool. | Log Display Ack | IxB | Tool
2500 | Error | Tensioner puller bar max number | Tensioner puller bar must be replaced. System is locked for usage. Pressure can only be released. | Send the tensioner to service organization for replacement of the puller bar. | Log Display Ack | Power Focus HC | Tool
2501 | Error | Pump motor protection alarm | The pump motor protection has stopped the motor. The system must stop. If the system is under pressure, it needs manual actions to release pressure. | Turn off the system. If under pressure, mechanically release the pressure and send the pump to service. | Log Display Ack | Power Focus HC | Tool
2502 | Error | Pump motor oil level low alarm | The pump motor oil level is low which has stopped the motor. If the system is under pressure, it needs manual actions to release pressure. | Turn off the system. If under pressure, mechanically release the pressure and top up oil. | Log Display Ack | Power Focus HC | Tool
2503 | Error | Pump motor oil temperature high alarm | The pump motor oil temperature is high. | Turn off the system and wait for the oil to cool down. | Log Display Ack | Power Focus HC | Tool
2504 | Error | Tensioner pressure sensor alarm | Failure in the pressure sensor electronics of the tensioner. No pressure can be read nor reported to the system. | Turn off the system. If under pressure, mechanically release the pressure and send the tensioner to service. | Log Display Ack | Power Focus HC | Tool
2505 | Error | Pump pressure sensor alarm | Failure in the pressure sensor electronics of the pump. No pressure can be read nor reported to the system. | Turn off the system. If under pressure, mechanically release the pressure and send the pump to service. | Log Display Ack | Power Focus HC | Tool
2506 | Error | Unexpected clockwise rotation detected | A clockwise nut rotation while waiting for pressure release after completed tensioning. The result is invalidated. | Release pressure and tension the nut again. | Log Display Conf | Power Focus HC | Tool
2507 | Error | Unexpected counter clockwise rotation detected | A counter clockwise nut rotation while waiting for pressure release after completed tensioning. The result is invalidated. | Release pressure and tension the nut again. | Log Display Conf | Power Focus HC | Tool
2508 | Error | Pump or tensioner pressure sensor failure | Too large difference between the pressure sensor readings in the pump and the tensioner. Pressurization is halted. | Problem in the hydraulics or the calibration of the pressure sensors. Restart the system and try again. If the problem repeats, contact your local Atlas Copco sales representative. | Log Display Ack | Power Focus HC | Tool
2509 | Error | Tensioner pressure sensor failure or hydraulic hose failure | The tensioner's pressure sensor indicates no pressure but the pump's sensor reads a pressure increase. Pressurization is halted. | Problem in the hydraulics or the calibration of the pressure sensors. Restart the system and try again. If the problem repeats, contact your local Atlas Copco sales representative. | Log Display Ack | Power Focus HC | Tool
2510 | Error | Set custom ID failed | Setting custom ID failed. | Restart the system and check the connected devices. If Custom ID for the unit is wrong, redo the setting. | Log Display Ack | Power Focus HC | Tool
2511 | Info | Custom ID is set | Setting custom ID succeeded. |  | Log Display Ack | Power Focus HC | Tool
2512 | Warning | Malformed Barcode string, ignored | The scanned string could not be parsed as a tower data bar code. | Scan a proper tower data qr code or scan tower section id. | Log Display Ack | Power Focus HC | Tool
2513 | Error | No pump pressure detected | The system is trying to pressurize but no pressure increase is registered in the pump. Possible cause is incorrect phase order in the three phase connector. | Power off the system and reverse the phases of the power connector. | Log Display Ack | Power Focus HC | Tool
2514 | Warning | Tensioner overtorque alarm | Too high torque is applied to the click wrench. This causes damage to the torque sensor. | Relax the torque. | Log | Power Focus HC | Tool
2515 | Warning | Tensioner overpressure alarm | The pressure in the tensioner is too high. | Let the pressure drop, or release the pressure. Check the hydraulic pressure parameters. | Log | Power Focus HC | Tool
2516 | Warning | Unexpected Pump or Tensioner firmware | Unexpected Pump or Tensioner firmware version detected, restart system. If the problem persists, the system may be possible to run, but carefully observe any unexpected behaviour. | Power cycle system | Log Display Ack | Power Focus HC | Tool
2517 | Error | Incompatible Pump or Tensioner firmware version, restart system. The system cannot run. | Incompatible Pump or Tensioner firmware version, restart system. The system cannot run. | Restart system, if this doesn’t help replace the failing unit. Check connected devices to see which one has not connected. | Log Display Ack | Power Focus HC | Tool
2518 | Error | Physical safety signal failed. | Safety signal from the hand controller has not reached the pump | Check the cable connected to the tensioner If the event re occurs contact service | Log Display Ack | Power Focus HC | Tool
2519 | Error | System entered fail safe mode | Fail safe mode activated | User acknowledgment required | Log Display Ack | Power Focus HC | Tool
2520 | Error | System exits fail safe mode | Fail safe mode deactivated | System returns to normal function | Log Display Ack | Power Focus HC | Tool
2523 | Error | Communication lost with the tensioner | Communication lost with the tensioner | Check the cable connected to the tensioner Event can occur when the system is powered off | Log Display Ack | Power Focus HC | Tool
2524 | Error | Communication lost with the pump | Communication lost with the pump | . Check the cables are connected Event can occur when the system is powered off | Log Display Ack | Power Focus HC | Tool
2525 | Error | Action requested from the hand controller is not performed by the pump | Action requested from the hand controller is not performed by the pump | Try again If this event occurs often contact service. | Log Display Ack | Power Focus HC | Tool
2800 | Error | There is an error on the clutch sensor | Check sensor and clutch assembly | If this event occurs often contact service. | Log Display Ack | Power Focus 6000 Power focus 8 | Tool
2801 | Error | Triggered when clutch settings alarm is enabled in settings and the current time is greater than next clutch settings date | Indicates that clutch settings of tool is needed | If this event occurs often contact service. | Log Display Ack | Power Focus 6000 Power focus 8 | Tool
3000 | Error | Controller Internal Software Error | Software error in the controller. | Contact service. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Controller
3001 | Error | Controller Clock Battery Empty | Internal battery is getting close to end of life. | Replace battery. | Log Display Ack Conf | Flex Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC | Controller, Drive and Synchronized tightening
3002 | Error | Drive Internal Software Error | Software error in the drive. | Contact service. | Log Display Conf | Flex Synchronized tightening | Drive
3010 | Warning | System Overheated | The controller is overheated. | Cool down. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and Synchronized tightening
3011 | Warning | Drive Overheated Controller Hardware |  | Cool down. | Log Display Conf | Flex ToolsControl | Controller, Drive and Synchronized tightening
3013 | Warning | Usage Limited Due To High Controller Temperature | Temperature limit value has been reached. Tightening has been inhibited to reduce risk for controller shutting down due to overheating. | Wait until controller temperature has been reduced. | Log Display Conf | Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC | Controller, Drive and Synchronized tightening
3020 | Warning | Controller Hardware Failure |  |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC | Controller, Drive and Synchronized tightening
3021 | Warning | System Voltage Problem | DC voltage too high or too low. |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC | Controller, Drive and Synchronized tightening
3022 | Warning | Controller Voltage Problem: AC Input Voltage Too High | DC voltage too high or too low. | Fix the input voltage. | Log Display | Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC | Controller, Drive and Synchronized tightening
3023 | Warning | Controller Voltage Problem: AC Input Voltage Too Low | DC voltage too high or too low. | Fix the input voltage. | Log Display | Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC | Controller, Drive and Synchronized tightening
3024 | Warning | Drive Voltage Problem: AC Input Voltage Too High | DC voltage too high or too low. | Fix the input voltage. | Log Display | Flex ToolsControl | Controller, Drive and Synchronized tightening
3025 | Warning | Drive Voltage Problem: AC Input Voltage Too Low | DC voltage too high or too low. | Fix the input voltage. | Log Display | Flex ToolsControl | Controller, Drive and Synchronized tightening
3026 | Info | Max number of IxB Connect tools already connected. | Indicates that the number of IxB Connect tools connected to the controller has reached the max. allowed connected tools. |  | Log | ToolsControl | Controller and Tool
3029 | Info | The client lost network connection | The tool has lost the network connection by either leaving the network coverage or due to another cause. | Troubleshoot by checking the roaming threshold and reduce the selected channel numbers to less than 24 to make sure roaming is enabled. | Log Display Conf Ack | IxB | Controller and Tool
3030 | Error | IP Address Conflicting With Another Node On The Network | The set IP address is in use by another device on the same network. | Change IP address on one of the devices. | Log Display Conf | Flex Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC Power Focus HC | Controller, Drive and Synchronized tightening
3031 | Info | Network Cable Unplugged | The carrier of the factory port is lost (cable disconnected). | Check the cable connection. | Log Display Conf | Flex Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC | Controller, Drive and Synchronized tightening
3032 | Info | Pairing Started | Tool pairing started. |  | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and Synchronized tightening
3033 | Info | Pairing Successful | Tool pairing successful. |  | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and Synchronized tightening
3034 | Info | Pairing Unsuccessful: No Tool Found | The controller found no tool to pair with when scanning for radio peers. | Set the tool in pairing mode and try again. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and Synchronized tightening
3035 | Error | Pairing Unsuccessful: More Than One Tool Found | The controller found more than one tool when scanning for radio peers. | Ensure that only one tool is in pairing mode when starting the pairing mode on the controller. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and Synchronized tightening
3036 | Error | Pairing Unsuccessful: Communication Error | The controller experienced a loss of connection, an unexpected answer or timeout during the pairing process. | Try to perform pairing one more time. If it fails again, service the tool. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and Synchronized tightening
3037 | Info | Pairing Unsuccessful: Tool Slot Is Full |  | Clear one tool slot. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC | Controller, Drive and Synchronized tightening
3040 | Warning | Emergency Stop | Drive disabled due to emergency stop. | Reset emergency stop. | Log Display Conf | Flex Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Controller, Drive and Synchronized tightening
3050 | Info | System Clock Updated | System clock has been updated. |  | Log Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC Power Focus HC | Controller, Drive and Synchronized tightening
3051 | Error | System Clock Error | Wrong time read from hardware Real Time Clock (RTC). | Change RTC battery. | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC Power Focus HC | Controller, Drive and Synchronized tightening
3052 | Warning | Remote Start Configuration Error | Mismatch between HW and SW remote start configuration. | Verify that HW dip switch matches the selected start source. | Log Display Conf | Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Controller, Drive and Synchronized tightening
3053 | Info | Drive Connected | Synchronized tightening drive has been connected. |  | Log Display | Flex Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Controller, Drive and Synchronized tightening
3054 | Info | Drive Disconnected | Drive disconnected from controller. | Check cabling and power-supply for externally connected drives or replace the controller. | Log Display | Flex Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Controller, Drive and Synchronized tightening
3055 | Warning | Mode Configuration Error | Generated when selected mode is configured wrongly. E.g. configuring two bolts with the same bolt number or the same channel, incomplete mode configuration. | Check ToolsTalk 2 for mode configuration error. | Log Display | Flex Synchronized tightening | Controller, Drive and Synchronized tightening
3056 | Warning | Unable to Start: Tool Or Drive Is Missing | Generated when a used channel is missing a drive or tool. | Verify Channel Menu on the HMI. Connect missing drive or tool. | Log Display | Flex Synchronized tightening | Controller, Drive and Synchronized tightening
3057 | Info | Unable to Start: Channel Is Already In Use | Generated when a needed channel has been allocated to another virtual station. |  | Log Display | Flex | Controller, Drive and Synchronized tightening
3058 | Info | No Mode Selected |  | Select mode. | Log Display | Flex Synchronized tightening | Controller, Drive and Synchronized tightening
3059 | Warning | Failed To Connect To Atlas Copco License Manager | Indicates that the controller failed to connect to the local license manager to get licenses. | Verify the local network. If it fails again, service the controller. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Controller, Drive and Synchronized tightening
3060 | Error | Number of Virtual Station licenses is exceeded. | Virtual Station license greater than available licenses. | Update licenses or Virtual Station configuration. | Log Display Ack | ToolsControl | Controller
3061 | Warning | Unable To Start: Enable Signal Is Low |  | Ensure the signal "Enable Operation" is set to high before tightening is started. | Log Display | Flex Synchronized tightening | Controller, Drive and Synchronized tightening
3062 | Warning | Unable To Start: Stop Signal Is High |  | Ensure the signal "Enable Operation" is set to low before tightening is started. | Log Display | Flex Synchronized tightening | Controller, Drive and Synchronized tightening
3063 | Warning | Unable To Start: All Channels Inhibited | All channels have been set inhibited, so no tightening can be started. | Set at least one channel to not be inhibited. | Log Display | Flex Synchronized tightening | Controller, Drive and Synchronized tightening
3064 | Warning | Carrier Number Faulty | A FlexCarrier hex switch is set to zero. | Turn the switch to a non-zero value. | Log Display | Flex | Controller, Drive and Synchronized tightening
3065 | Warning | Carrier E-Stop Configuration Plug Wrong Type Or Missing | A Carrier is missing its E-stop configuration plug, or the plug type is wrong. | Insert correct plug type. | Log Display | Flex | Controller, Drive and Synchronized tightening
3066 | Warning | Carrier Voltage Inlet: No 3-Phase AC |  | Ensure the 3-phase power to the carrier is within acceptable limits and fully functional. Ensure the 3-phase cables are in good condition and properly connected. | Log Display | Flex | Controller, Drive and Synchronized tightening
3067 | Warning | Carrier Voltage Inlet: One AC Phase Missing |  | Ensure the 3-phase power to the carrier is within acceptable limits and fully functional. Ensure the 3-phase cables are in good condition and properly connected. | Log Display | Flex | Controller, Drive and Synchronized tightening
3068 | Warning | Carrier: Internal 24 VDC Power Supply Unit Broken |  | Service the carrier. | Log Display | Flex | Controller, Drive and Synchronized tightening
3069 | Warning | Carrier 24 Voltage OUT-Port Disabled Due To Over-Current |  | Reset the system. | Log Display | Flex | Controller, Drive and Synchronized tightening
3070 | Warning | Carrier, Hardware Error In PF6 FlexControl Cable OUT |  | Reset the system. | Log Display | Flex | Controller, Drive and Synchronized tightening
3071 | Warning | Carrier, Hardware Error In PF6 FlexControl Cable IN |  | Reset the system. | Log Display | Flex | Controller, Drive and Synchronized tightening
3072 | Warning | Emergency Stop 24 VDC Power Failure Due To Short-Circuit |  | Service the carrier. | Log Display | Flex | Controller, Drive and Synchronized tightening
3073 | Warning | Unable To Start: System Is Emergency Stopped | When allocating multiple spindles, this event is invoked by "preStartCheckFailed" due to emergency stop. | Reset the emergency stop. | Log Display | Flex Synchronized tightening | Controller, Drive and Synchronized tightening
3074 | Warning | Carrier Overheated |  | Cool down. | Log Display | Flex | Controller, Drive and Synchronized tightening
3075 | Warning | Carrier Temperature OK |  |  | Log Display | Flex | Controller, Drive and Synchronized tightening
3076 | Warning | Carrier: Internal 24 VDC Power Supply Overload | Current output from internal PSU is too high. | Disconnect other carriers that are powered from the PSU. Disconnect any external equipment using 24 VDC. | Log Display | Flex | Controller, Drive and Synchronized tightening
3077 | Warning | Carrier: Internal 24 VDC Power Supply Over Voltage | Voltage output from internal PSU is too high. | Replace the carrier. | Log Display | Flex | Controller, Drive and Synchronized tightening
3078 | Warning | Carrier: Internal 24 VDC Power Supply Under Voltage | Voltage output from internal PSU is too low. | Replace the carrier. | Log Display | Flex | Controller, Drive and Synchronized tightening
3079 | Warning | External Supply To Carrier: 24 VDC Over Voltage | Backup input voltage is more than 27 VDC. | Adjust the backup input voltage. | Log Display | Flex | Controller, Drive and Synchronized tightening
3080 | Warning | External Supply To Carrier: 24 VDC Under Voltage | Backup input voltage is less than 19 VDC. | Adjust the backup input voltage. | Log Display | Flex | Controller, Drive and Synchronized tightening
3081 | Warning | Carrier Voltage Inlet: 3-Phase AC Over Voltage | Input voltage is too high. | Lower input voltage: must be 400 VAC or 480 VAC. | Log Display | Flex | Controller, Drive and Synchronized tightening
3082 | Warning | Carrier Voltage Inlet: 3-Phase AC Under Voltage | Input voltage is too low. | Higher input voltage: must be 400 VAC or 480 VAC. | Log Display | Flex | Controller, Drive and Synchronized tightening
3083 | Error | Wrong Anybus/Profisafe Module Firmware |  | Update the firmware in the anybus module to the latest version. | Log Display | Flex Power Focus 6000 Power Focus 8 Synchronized tightening | Controller, Drive and Synchronized tightening
3084 | Error | Soft PLC Runtime Error | eCLR has terminated in an uncontrolled way. |  | Log Display Conf | Flex Power Focus 6000 Power Focus 8 Synchronized tightening | Controller, Drive and Synchronized tightening
3085 | Warning | Carrier: Fan Module Out Of Order |  | Replace fan module. | Log Display | Flex | Controller, Drive and Synchronized tightening
3086 | Warning | Carrier: Fan Module Partly Out Of Order |  | Replace fan module. | Log Display | Flex | Controller, Drive and Synchronized tightening
3087 | Warning | Carrier: Left Fan Module Out Of Order |  | Replace fan module. | Log Display | Flex | Controller, Drive and Synchronized tightening
3088 | Warning | Carrier: Left Fan Module Partly Out Of Order |  | Replace fan module. | Log Display | Flex | Controller, Drive and Synchronized tightening
3089 | Warning | Carrier: Right Fan Module Out Of Order |  | Replace fan module. | Log Display | Flex | Controller, Drive and Synchronized tightening
3090 | Warning | Carrier: Right Fan Module Partly Out Of Order |  | Replace fan module. | Log Display | Flex | Controller, Drive and Synchronized tightening
3091 | Info | Sync member channel collision | Generated when two or more sync members are configured to the same channel. | Reconfigure the colliding sync member to have a unique or different channel that has not been allocated to another sync member. | Log Conf Display Ack | Power Focus 8 Synchronized tightening ToolsControl | Controller, Drive and Synchronized tightening
3093 | Warning | Digital input received before the trigger is pressed. | Indicates that something went wrong with setup. |  | Log Conf Display Ack | Power Focus 8 Synchronized tightening ToolsControl | Controller, Drive and Synchronized tightening
3095 | Warning | WiFi Signal Strength Low | The wireless network signal strength is below the value set in setting "Warn on signal strength below (dBm)". |  | Conf | IxB | Controller and Tool
3096 | Warning | Cellular signal strength low | The RSSI value for the cellular connection is under the defined threshold value of -98 dBm. | Move the tool closer to the cellular antennas for a stronger connection and avoid data loss. | Conf | IxB | Controller, Drive and Synchronized tightening
3097 | Warning | Cellular connection lost | The system lost connection to the cellular network. | Move the tool closer to the cellular antennas. Check the cellular connection setup so correct APN is still configured. Check the cellular network for any problems. | Log Display Conf | IxB | Controller, Drive and Synchronized tightening
3100 | Warning | Mode Configuration Does Not Exist |  | Select an existing sync mode before starting a tightening. | Log Display | Flex Synchronized tightening | Controller, Drive and Synchronized tightening
3150 | Error | Software IAM Incompatibility | IAM is incompatible with the software that is installed on the controller. | Replace IAM. | Log Display Ack | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC | Controller, Drive and Synchronized tightening
3160 | Error | Failed To Activate Newly Installed Software | Something went wrong during the activation. When the newly installed software starts, a fallback to the previous working software happens. This error happens when the new software fails to start for three times and only during software installation. | Take an export and contact Atlas Copco for further assistance. Note down the software version you are trying to install as well as the software version that is working. | Log Display Ack | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC | Controller, Drive and Synchronized tightening
3161 | Error | Started On Unexpected Software Partition | The controller has started on the inactive software side and not on the expected software side. | Note down the software information (on the Home screen of the controller, select Controller > Software). Try to restart the controller and make sure its running on correct software when started again. If error persists, do an export and contact Atlas Copco. | Log Display Ack | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC | Controller, Drive and Synchronized tightening
3162 | Info | Software Upgrade Verification Failed | Failed to verify the integrity and authenticity of the software package. | Ensure that the software package that is being upgraded to is a signed, software package. Note down the software information (on the Home screen of the controller, select Controller > Software). If error persists, do an export and contact Atlas Copco. | Log Display Ack | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC | Controller, Drive and Synchronized tightening
3180 | Info | Software Adapter Import Verification Failed | Failed to verify the integrity and authenticity of the imported protocol adapters. | Make sure that the protocol adapters that are being imported are signed, protocol adapters. If error persists, do an export and contact Atlas Copco. | Log Display Ack | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC | Controller, Drive and Synchronized tightening
3500 | Error | Generic License Manager Error | Inconsistency detected in the feature management system used. | Contact Atlas Copco representative. | Log Display Ack | IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Controller, Drive and Synchronized tightening
3501 | Error | License Manager Synchronization Error | Synchronization with the license server failed. | Contact Atlas Copco service representative. | Log Display Ack | IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Controller, Drive and Synchronized tightening
3502 | Info | License Manager Synchronization Done | Synchronization with the license server completed. |  |  | IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Controller, Drive and Synchronized tightening
3503 | Warning | License Manager: Another Source in Use | License is used by another source. | Verify license assignment. | Log Display | IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Controller, Drive and Synchronized tightening
3504 | Warning | License Manager Restart Needed |  | Restart license manager. | Log Display | IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Controller, Drive and Synchronized tightening
3505 | Info | USB License Synchronization Started | Moving licenses from the USB license dongle started. |  | Log | Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl Power Focus HC | Controller, Drive and Synchronized tightening
3506 | Error | USB License Synchronization Error | Moving licenses from the USB license dongle failed. | Contact Atlas Copco service representative. | Log | Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl Power Focus HC | Controller, Drive and Synchronized tightening
3507 | Info | USB License Synchronization Done | Moving licenses from the USB license dongle done. |  | Log | Power Focus 6000 Power Focus 8 Power Focus HC | Controller, Drive and Synchronized tightening
3508 | Info | One or more of your licenses are about to expire. Please make sure you have a license server configured |  | Update licenses. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Controller, Drive and Synchronized tightening
3510 | Error | There is already a Local License Server in use. Return all licenses to the server prior to configuring a new one. | Inconsistency detected in a license to be used during configuration. | Update licenses. | Log Display Ack | ToolsControl | Controller
3511 | Warning | One of your licenses has a different license definition | Inconsistency detected in a license to be used. | Contact Atlas Copco representative. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl Power Focus HC | Controller, Drive and Synchronized tightening
3512 | Error | Unexpected license service error. Contact Atlas Copco for further assistance. |  | Contact Atlas Copco representative. | Log Conf Display Ack | ToolsControl | Controller
3550 | Warning | License Is Missing |  | Install the correct license. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl Power Focus HC | Controller, Drive and Synchronized tightening
3551 | Warning | Wireless Communication Disabled By Licensing |  | Unassign Standalone license from the Virtual Station. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Controller, Drive and Synchronized tightening
3600 | Info | System restart triggered by user | Restart is triggered as a consequence of a user action within the system, such as: After importing an export. Activating new software after software update. Swapping software side. Performing a service task that require a system restart. Open end tuning on IxB. Switching from WiFi to Bluetooth on IxB. |  | Log Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC Power Focus HC | Controller and Tool
3601 | Info | Unexpected system shut down | The system rebooted or shut down unexpectedly |  | Log Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC Power Focus HC ToolsControl | Controller and Tool
3610 | Info | System shut down due to power loss | Power switch is pressed or controller is disconnected from power source |  | Log Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC Power Focus HC ToolsControl | Controller and Tool
3611 | Info | Backup battery timer timed out, shutting down | Tool have been runnning on backup battery for more than 20s |  | Log Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC Power Focus HC ToolsControl | Controller and Tool
3612 | Info | System shut down due to inactivity | Inactivity timeout has expired |  | Log Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC Power Focus HC ToolsControl | Controller and Tool
4010 | Info | Tool Locked By Digital Input | The tool is locked by a digital input signal. |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tightening Process
4011 | Info | Tool Locked By Open Protocol | The tool is locked by Open Protocol. |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tightening Process
4012 | Info | Tool Locked By Fieldbus | The tool is locked by the Fieldbus. |  | Log Display Conf | Flex Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC | Tightening Process
4013 | Info | Tool Locked By Socket Selector | Tool is locked when the socket selector is disconnected from the Virtual Station. | Unlock by Master Unlock. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4014 | Info | Tool Locked By Soft PLC | Soft PLC signal locked the tool. | Unlock by Master Unlock. | Log Display Conf | Flex Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC | Tightening Process
4015 | Info | Loosening Disabled | Loosening is disabled in the tightening program. |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl XB | Tightening Process
4016 | Info | Tightening Disabled |  |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl XB | Tightening Process
4017 | Info | Loosening Not Configured | Loosening is not configured in the selected tightening program | Select different tightening program. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tightening Process
4020 | Info | Too Many NOK Tightenings | Maximum consecutive NOK tightenings in batch is exceeded |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tightening Process
4021 | Info | Too many consecutive loosenings | Maximum consecutive loosenings configured in General Virtual Station has been reached | An external input has to unlock and reset by signal Reset too many loosening lock or Master unlock. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Sync Power Focus XC ToolsControl | Group
4025 | Info | No Tightening Program Selected | No tightening program selected. | Select tightening program or batch sequence. | Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4030 | Info | Batch Sequence Aborted | The batch sequence has been aborted. |  | Log Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC Power Focus HC ToolsControl | Tightening Process
4031 | Info | Max Time To Complete Batch Sequence Reached |  |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tightening Process
4032 | Info | Max Time To Complete First Tightening Reached |  |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tightening Process
4035 | Info | Locked By Line Control |  |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4040 | Info | Locked By Alternative Identifier | Tool locked by alternative identifier. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4050 |  | Invalid Socket Configuration | Tightening program assigned to multiple sockets. | Tightening program assigned to multiple sockets. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4060 | Info | Tool Locked On Batch Complete | When running a batch with flag Tool lock on batch sequence complete this event is generated when the user press the trigger. | Unlock with signal Unlock Tool on complete. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tightening Process
4062 | Info | Tool Locked By Result Synchronization | Results from tool are being synchronized with the controller. | Wait until result sync is done to restart work. | Log Display Conf Ack | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tightening Process
4063 | Info | Tool Locked due to transducer redundancy error | Tool is locked due toredundancy error. |  | Log Display | Power Focus 6000 ToolsControl |
4064 | Info | Tool Locked by Automation Rules | Tool is locked by Automation rules. | No action | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl |
4065 | Info | Tool locked by test tightening | Tool is started when test tightening mode is active. | Exit test tightening | Log Conf Display | Flex Synchronized tightening | Tightening Process
4070 | Info | Process Enter Manual Mode | Indicates that manual mode has been activated for a virtual station. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4071 | Info | Process Enter Automatic Mode | Indicates that automatic mode has been entered for a virtual station. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4072 | Info | Test Bolt |  |  | Conf | Flex Synchronized tightening | Tightening Process
4073 | Info | Tool zero position updated | Indicates that the tool zero position is set using signals. |  | Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tightening Process
4100 | Warning | Identifier Not Accepted: Invalid String Length |  |  | Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tightening Process
4101 | Warning | String Selection Unsuccessful: Multiple Matches |  |  | Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tightening Process
4102 | Warning | String Selection Unsuccessful: No Match Found |  |  | Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tightening Process
4103 | Warning | Identifier Not Accepted: Identical String Already Received |  |  | Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tightening Process
4104 | Warning | Identifier Not Accepted: No Match Found |  |  | Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Tightening Process
4105 | Warning | Assembly task selection unsuccessful: No match found |  |  | Log Conf Display | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening ToolsControl | Controller
4106 | Warning | Assembly task selection unsuccessful: Multiple matches |  |  | Log Conf Display | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening ToolsControl | Controller
4107 | Warning | Wrong location for selected assembly task | The assembly work task has been configured to use device location to validate but not select assembly tasks. The selected assembly task is allowed to start when the controller/tool is at the expected location. | Move the controller to the expected work zone. | Log Conf Display | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening ToolsControl | Controller
4108 | Warning | The assembly work task has been deleted | The active assembly work task (selected in the virtual station) has been deleted. | Select the new/correct assembly work task as the task in the virtual station. | Log Conf Display | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening ToolsControl | Controller
4109 | Warning | The assembly task has already been completed |  |  | Log Conf Display | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening ToolsControl | Controller
4110 | Warning | The selected assembly task is uncompleted | New input has been provided to the controller suggesting that a new assembly task should be selected when one is already selected and in progress (i.e. at least one tightening has been performed). | Return to the work zone and complete the started assembly task or abort it to be able to select another assembly task. | Log Conf Display | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening ToolsControl | Controller
4111 | Warning | Invalid assembly task priorities | In the controller there are at least two different assembly tasks which are configured with the same priority value. This is not allowed if the assembly tasks are supposed to be selected together one after the other i.e. a multiselection. | Check the assembly task configurations. | Log Conf Display | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening ToolsControl | Controller
4112 | Warning | PAT build data has been requested | The assembly work task has been configured to request new PAT build data when an unknown product identifier is provided to the controller. Such a request has been made and while in progress the tool will be locked until it either succeeds or time out. | Wait for request to complete or time out. | Log Conf Display | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening ToolsControl | Controller
4113 | Warning | PAT build data is missing | The assembly work task has been configured to request new PAT build data when an unknown product identifier is provided to the controller. Such a request has been made and was unsuccessful i.e. the provided product identifier is still unknown. | Check PAT build data and data/logs in customer upper layer system | Log Conf Display | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening ToolsControl | Controller
4114 | Warning | External dependencies not ready | The assembly task has been configured to require clearance from a customer upper layer system before it is allowed to be selected. | Check PAT build data and data/logs in customer upper layer system | Log Conf Display | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening ToolsControl | Controller
4115 | Warning | No assembly task selected |  |  | Log Conf Display | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening ToolsControl | Controller
4116 | Warning | Assembly task aborted, process timer expired | The assembly task has been configured to use one or more process timers which will trigger an abort if not satisfied in time. See the assembly task configuration for more details. |  | Log Conf Display | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening ToolsControl | Controller
4117 | Warning | Assembly task resume error, abort required | The assembly task to resume (or the parent assembly work task) has been modified in such as way that it cannot be resumed. An abort is required to confirm this, which will then allow new assembly task selections to be made. | Preform an abort. On IXB tools this can be done in the batch operations menu the EHMI/RHMI. | Log Conf Display | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening ToolsControl | Controller
4119 | Warning | Assembly task not found | The list of assembly task IDs in the assembly work task contains at least one invalid ID (the corresponding assembly task does not exist in the controller). | Check the assembly work task configuration | Log Conf Display | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening ToolsControl | Controller
4120 | Warning | Assembly task configuration error | General error code for an unknown assembly task configuration error. | Check the assembly task configurations. See the worktask log for details. | Log Conf Display | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening ToolsControl | Controller
4121 | Warning | Tightening task not set for assembly task | An assembly task doesn't have a tightening task (tightening program or batch sequence etc.) configured. | Check the assembly task configurations. | Log Conf Display | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening ToolsControl | Controller
4122 | Warning | Tightening task not found for assembly task | The id of the configured tightening task in an assembly task is invalid (the corresponding tightening task doesn't exist in the controller). | Check the assembly task configurations. | Log Conf Display | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening ToolsControl | Controller
4123 | Warning | Assembly task has no joint ids | An assembly task is configured to use "Batch control - Joint id" but no joint ids have been configured and none can be found in the PAT build data. | Check the assembly task configurations and PAT build data. | Log Conf Display | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening ToolsControl | Controller
4500 | Info | Result DriveError | Internal driver error or driver loss detected. |  | Conf | Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4501 | Info | Result Rehit | Attempt to tighten an already tightened bolt when Rehit detection is on. | Step Category for the Start Stage must be set to Soft Start. | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4502 | Info | Result Soft Start Torque Low | Soft start torque below minimum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4503 | Info | Result Soft Start Torque High | Soft start torque exceeded maximum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4504 | Info | Result Self Tap Torque High | Self-tap torque exceeded maximum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4505 | Info | Result Self Tap Torque Low | Self-tap torque below minimum limit. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4506 | Info | Result Safety Torque Low | Automatically calculated torque value to ensure torque sensor is mounted correctly. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4507 | Info | Result Rundown Torque High | Rundown torque exceeded maximum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4508 | Info | Result Rundown Angle High | Rundown angle exceeded maximum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4509 | Info | Result Rundown Time High | Rundown time exceeded maximum limit. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4510 | Info | Result Rundown Time Low | Rundown time below minimum limit. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4511 | Info | Result Rundown Torque Low | Rundown torque below minimum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4512 | Info | Result Rundown Angle Low | Rundown angle below minimum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4513 | Info | Result Final Torque High | Final step torque exceeded maximum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4514 | Info | Result Final Angle High | Final step angle exceeded maximum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4515 | Info | Result Final Torque Low | Final step torque below minimum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4516 | Info | Result Final Angle Low | Final step angle below minimum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4517 | Info | Result Tightening Timeout | Tightening time limit exceeded. For General Tightening Strategies max tightening time is 30 seconds. For Multistep max tightening time depends on step restriction Maximum Time Limit. Error code is dependent on tightening stage. | Redo tightening. | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4518 | Info | Result Trigger Lost | Tool trigger was released before target was reached. For General Tightening Strategies it is not allowed to release the trigger before the tightening stage has finished. For Multistep, the error is displayed when trigger is lost before the target in a specific step is reached. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4519 | Info | Premature Torque Loss | Socket has slipped off the nut. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4520 | Info | Result Target Reached Before Final Step | Target torque reached before final step in tightening program. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4521 | Info | Result Post View Torque Low | Post view torque below minimum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4522 | Info | Result Post View Torque High | Post view torque exceeded maximum level. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4523 | Info | Result Post View Torque Interval Not Reached | Post view torque interval not reached. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4524 | Info | Result Torque Compensation Interval Not Reached | Torque compensation interval angle before rundown end not reached. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4525 | Info | Result Tool Movement Exceeded | From a NOK tightening detailed status. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4526 | Info | Result SafetyCurrMon Sensor Mismatch | Current monitoring error. |  |  | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4527 | Info | Result Tool Movement Exceeded |  |  |  | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4538 | Info | Result Final Supervision Torque Low | Final Supervision Torque was not reached. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4543 | Info | Result Snug Monitor High | Wrench only. Monitor detected snug value exceeded. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4545 | Info | Result No Residual Torque | Wrench only. Residual torque was under threshold. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4546 | Info | Result Overspeed | Wrench only. Wrench gyro failed to measure angle due to high speed. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4547 | Info | Result Effective Loosening | Wrench only. Wrench detected unexpected loosening. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4548 | Info | Result Final Less Than Target | Final torque is below target torque set in tightening program. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4549 | Info | TurboTight Time Limit Exceeded |  |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4550 | Info | Result Rundown Pulses High | Maximum number of rundown pulses is exceeded. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4551 | Info | Result Rundown Pulses Low | Rundown is completed before the minimum number of rundown pulses is reached. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4552 | Info | Result Final Pulses High | Maximum number of pulses is exceeded. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4553 | Info | Result Final Pulses Low | Tightening is completed before the minimum number of pulses is reached. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4554 | Info | Current At Shutoff High | Current at shut off exceeded Current Limit High. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4555 | Info | Current At Shutoff Low | Shut off current measured was below Current Limit Low. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4556 | Info | Uncategorized Multistep Error | An error in the multistep configuration, often with tool validation. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4557 | Info | Result Overload |  |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4559 | Info | Result Stopped | The event is triggered when an external stop signal or lock signal is aborting an ongoing tightening. The event is introduced to distinguish between trigger loss and external stop. |  | Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Tightening Process
4600 | Warning | Data Drop or Data Hold used in combination with Batch Tightening. The signals have no effect |  | Data Drop and Data Hold are only supported for worktasks, without batch control. Select another worktask if the signals must be used. |  | Flex Synchronized tightening | Tightening Process
4601 | Info | Data Hold Active: tightening result is sent once signal is low |  |  |  | Flex Synchronized tightening | Tightening Process
4602 | Info | Data Drop active: tightening result discarded |  |  |  | Flex Synchronized tightening | Tightening Process
5010 | Warning | Invalid Tightening Program Parameter Value | The parameter in the selected tightening program are invalid. | Check the configuration of the selected tightening program to find and to change the value of the parameter. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC Power Focus HC ToolsControl | Program Configuration
5011 | Warning | Couldn't prepare program storage in tool | It is not possible to read the current program storage size in the tool, or to prepare the program storage for downloading the updated, or newly selected program to the tool. | Check the tool for supported software version. Reboot the tool. Select the tightening program again. Check network connection for data consistency and quality. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Program Configuration
5020 | Info | Main Trigger Is Not The Active Start Source | Generated when configured for push start only and user presses main trigger. Will be generated until user presses the push start. | Press push start to start the tool. | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Program Configuration
5030 | Info | Tightening Program Complexity Exceeds Tool Capacity | The selected tightening program is too complex for the STB tool that is used. Tool will be locked. | Reduce complexity of the tightening program, or choose different program. | Log Display Conf | Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Program Configuration
6010 | Info | Accessory Connected | Accessory is connected to the controller. |  | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Accessory
6020 | Info | Accessory Disconnected | Accessory is disconnected from the controller. |  | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Accessory
6021 | Warning | Fieldbus Offline | No communication with Fieldbus. |  | Log Display Ack Conf | Flex Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC | Accessory
6030 | Warning | Accessory Address Collision | Two or more accessories with the same address are connected. | Change address on accessory. | Log Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Accessory
6040 | Warning | Accessory Communication Error | Intermittent communication error with accessory. | Check cables and connectors. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Accessory
6041 | Warning | Fieldbus Error | Communication error with Fieldbus. |  | Log Display Ack Conf | Flex Power Focus 6000 Power Focus 8 Synchronized tightening | Accessory
6042 | Warning | Fieldbus Module Mismatch | The installed Fieldbus module does not match with the configured module. | Change the configuration to match with the installed module, or replace the installed module with the correct one. | Log Display Ack Conf | Flex Power Focus 6000 Power Focus 8 Synchronized tightening | Accessory
6043 | Warning | Fieldbus Output Buffer Overflow | The output buffer used for the Fieldbus communication is exhausted and an overflow of the buffer has occurred. One or more signal updates have been discarded. | Stop Fieldbus communication and Fieldbus diagnostics (if used) to recover the buffer. If this event occurs frequently, check your Fieldbus communication setup, including the PLC program: too frequent updates compared to your update interval can lead to this scenario. | Log Display Ack Conf | Flex Power Focus 6000 Power Focus 8 Synchronized tightening | Accessory
6044 | Warning | Fieldbus Provider ID mismatch | The installed Fieldbus module is not supported. | Connect a supported Atlas Copco fieldbus module. | Log Display Ack | Power Focus 8 | Accessory
6050 | Info | Wrong Socket Selected | Generated when no or incorrect socket is selected. |  | Log Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Accessory
6090 | Warning | Barcode Scanner Could Not Be Identified | When no unique serial number is found. | Configure the barcode reader device. | Log Display Ack Conf | Flex Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC Power Focus HC | Accessory
6500 | Warning | Invalid Rule Configuration | Rule configuration is invalid if the virtual station mapped does not exist, invalid cease configuration or if the rule has no triggers or no actions | Verify the configuration of the tool. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl |
6501 | Warning | Rule Triggered While Running | Running rule is re-triggered by the same trigger. | Disable and enable the rule. | Log Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl |
6502 | Info | Failed to execute Action | Rule fails to execute an event when it cannot perform an action on a deleted or non-existent virtual station. This occurs when the virtual station configured for the rule has been removed. | Action is corrected rule is disabled and enabled. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl |
6503 | Warning | Running Rule Deleted | This event occurs if a currently running rule is deleted. The action will not be reset if running rule is deleted. | No action. | Log Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl |
6504 | Warning | Running Rule Disabled | This event occurs if a currently running rule is disabled. The action will not be reset if running rule is disabled. | No action. | Log Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl |
6505 | Warning | Running Rule Updated | Running rule updated event if a currently running rule is updated. | No action. | Log Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl |
7010 | Info | Message Text To Display | General event for displaying of messages. |  | Display Ack Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC Power Focus HC ToolsControl | Message
8135 | Info | Machine capability test mode activated | Machine capability test mode has been activated. The mode allows targeted steps within a multistage configuration to not be executed while the mode is active. | Activate Machine capability test mode. | Log Conf Display Ack | Power Focus 6000 Power Focus 8 Flex Power Focus XC IxB XB | Controller
8136 | Info | Machine capability test mode deactivated | Machine capability test mode has been deactivated. All steps within a multistage program will be executed as normal. | Deactivate Machine capability test mode. | Log Conf Display Ack | Power Focus 6000 Power Focus 8 Flex Power Focus XC IxB XB | Controller
8200 | Info | Failed To Open Serial Port | Serial port to be used could not be opened. | Check serial port connections. | Display Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC | Miscellaneous
8300 | Warning | Open Protocol client communication timed out | Communication to an Open Protocol client has timed out. No keep alive message or command sent within expected time. | Check controller network connection. Check network setup: firewall and switches. Check client side application software. | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC ToolsControl | Miscellaneous
8214 | Error | EHMI Software Version Mismatch | EHMI software version does not match in compatibility with the controller. | Update the software version of the EHMI. | Log Display Ack Conf | IxB Power Focus 6000 Power Focus 8 Power Focus XC ToolsControl | Miscellaneous
8400 | Info | Controller event | Deleted configuration history. |  | Log Display Conf | Flex IxB Power Focus 6000 Power Focus 8 Synchronized tightening Power Focus XC Power Focus HC ToolsControl STRw Sync | Controller

## Glossary

Conf - Event Codes list

Tells the user whether it is possible to configure the event through the "Configure Event" page.

Available for - Event Codes list

List of products for which the event code is available.

Groups - Event Codes list

Group which the event codes belong to.

Event Description

A short description of the event and why it occurs.

Procedure - Event Codes list

If applicable, the procedure contains an instruction on how to clear the event.

Log - Event Codes list

Tells the user whether the event is to be saved in the event log or not. The value in this list is the default value.

display - Event Codes list

Tells the user whether the event is to be displayed on the screen or not. The value in this list is the default value.

Ack - Event Codes list

Tells the user whether the event must be acknowledged or not before you can proceed. The value in this list is the default value.

Event code

The unique event number.

Type of events - Event Codes list

Type of event: Info, Warning, and Error.

Event name

A descriptive name of the event.