# Fieldbus parameters for CC Link

The table below only lists specific parameters for CC Link. For the general parameters, see Fieldbus Parameters General.

Field | Description | Default value
--- | --- | ---
Baud rate | Speed of the communication link. Select speed from the drop-down menu. 156 kbps; 625 kbps; 2500 kbps; 5 Mbps; 10 Mbps. | 156 kbps
Fieldbus node address | A unique address for each separate unit within the network |
Version | Version 1: By default, the module automatically calculates the required number of Occupied Stations based on the mapped Process Data. Version 2: By implementing the Network Settings in the CC-Link, it is possible to customize the implementation for CC-Link Version 2 and use larger data sizes through Extension Cycles. |
Occupied stations | A parameter setting which is dependent on which Version has been chosen. This is used in combination with the Extension Cycles parameter. |
Extension cycles | Parameter setting used for sending larger data sizes, used in combination with the Version and Occupied Station parameters. |

Relevant Information

- Fieldbus Parameters General
- Fieldbus Parameters General