# Configuring the Remote Logging Connection

To connect a controller to a remote logging server, configure and activate the remote logging settings on the controller:

1. Select a controller in the Plant structure .

2. Go to Settings .

   The workspace area displays the Settings menus.

3. On the Remote Logging section, configure the following parameters:

   Field | Description
   --- | ---
   On/Off | Enables/Disables communication with the remote logging server
   Protocol | Selects TCP or UDP protocol
   Server host | Remote logging server IP address
   Server port | Remote logging server port

4. Select the applicable log level(s) for each facility:

   Log level | SysLog classification
   --- | ---
   Error | Alert, Critical, Emergency, Error
   Warning | Warning
   Info | Informational, Notice

5. Select Set to apply the configurations on the controller.