# Operator Panel

The Operator Panel is connected to the I/O bus and provides a configurable digital communication link between an operator and the controller. Lamps, buttons, buzzers and switches are used in the communication. Read the operator panel documentation for address configuration and specifications of connections.

How to assign an accessory configuration to a Virtual Station is described in the Virtual Station section.

Relevant Information

- Adding an accessory to a Virtual Station
- Unassigning an Accessory from a Virtual Station