# Validating the Client-Server Installation

After successful installation of the client-server version of the ToolsTalk 2 application, a controller is needed for a complete system test.

- The server computer must be connected to the network.

- The client computer must be connected to the network.

- The controller must be connected to the network and configured to communicate with the server computer.

- Check that Atlas Copco Data Communication service is started.

The server and client may be installed on the same computer.

- For configuration and starting the controller please refer to the controller user guide.

- For configuration, starting and navigating in the ToolsTalk 2 GUI, please refer to the ToolsTalk 2 user guide.

If the ToolsTalk 2 client is installed, the application can be started in the following way:

- Select the Windows Start menu and locate the ToolsTalk 2 folder.

- Select the ToolsTalk 2 icon to launch the application.

Relevant Information

- Getting started