# Tool Configuration - Buzzer

The Buzzer can be configured to emit different sounds. Output signals can be mapped to each of the signals and provides an audio interface to the operator.

The Buzzer is located on the tool and is configured as a tool accessory.

Command | Description
--- | ---
Add | Add a new sound configuration to the table.
Delete | Remove one or more selected sound configurations.

Up to 20 different signals can be mapped to a sound and each sound can have its own characteristic profile, with parameters described in the table below.

Parameter | Description
--- | ---
Check box | Selects a row in the table.
Signal | Select a signal that triggers the sound.
Frequency | Exact frequency in Hz.
Time on | Time (in ms) that the buzzer emits a sound.
Time off | Time (in ms) that the buzzer is quiet.
Repetition | Number of times the buzzer repeats the on/off sequence.
Volume | The buzzer volume, in percentage of max volume.
Priority | 10 different priority levels are available for the sounds where one (1) is the highest priority level. Default priority level is five.

For two simultaneous signals, the signal with highest priority overrides the other signal.

A buzzer signal runs until termination and is not interrupted by a higher prioritized signal.