# Socket Selector Control Switch

The Control switch has two positions:

Position | Description
--- | ---
Auto | The controller controls the LED lamps on the Socket Selector, which guide the operator to the correct socket selection.
External | The controller has no control of the socket selector. All functionality of the LED lamps is controlled by an external control system through the Open Protocol communication or by the Fieldbus module.