# Fieldbus parameters for DeviceNet

The table below only lists specific parameters for DeviceNet. For the general parameters, see Fieldbus Parameters General.

Field | Description | Default value
--- | --- | ---
Fieldbus node address |  |
Baud rate | Speed of the communication link. Select speed from the drop-down menu. 125 kbps; 250 kbps; 500 kbps, Automatic. | Automatic
Connection mode | Select the type of communication between the fieldbus master (PLC) and the subordinate controller. Select from a drop-down menu: Polled Bitstrobe Change of state | Polled

Relevant Information

- Fieldbus Parameters General
- Fieldbus Parameters General