# Fieldbus Virtual Station Mapping Configuration

A virtual station in a controller and the fieldbus master communicate by exchanging a fieldbus map between each other.

One or more fieldbus maps are combined into a Process Data Frame, which is sent on the physical communication link between the controller and the fieldbus master.

Fieldbus Virtual Station Mapping Configuration
Column | Function
--- | ---
Check box | Select or deselect a mapping.
Virtual station | Name of virtual station.
Fieldbus configuration | The fieldbus map.
To/From controller offset | Starting point of the fieldbus map within the Process Data Frame.

Relevant Information

- Pushing Configurations to a Controller