# Active Identifier String 3 - 190

Signal corresponding to the third configured string in Source batch-string.
Active Identifier String 3 signal is sent once a scanning sequence is done and a sequence has been selected, thus the identifier parts are active.
The strings is filtered with saved position.
Only sent when running Source batch string.

Name in SoftPLC: ACTIVE_ID_STRING_3

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | String | 8 | 800
IdentifierU32Hnw | State | String | 8 | 800
IdentifierU32 | State | String | 8 | 800

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: FALSE

- Operator Panel: FALSE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: FALSE

- TLS Tag: FALSE

- I/O Expander: FALSE