# Configure Acyclic Data

The Configure Acyclic Data area displays the visualization of the acyclic configuration set by max size, offset and template size. All configurations are in the byte level.

The acyclic data frame displayed on the left changes when items are added to the common, bolt or channel area.

If the values of offset and template size are zero, the common, bolt or channel area is greyed out and non-editable.

## Data in the Common Area

The common area contains data that is global and is applicable to all the spindles in the same station. The common area data is displayed after the header and before the bolt/channel data.

## Bolt or Channel Data

The data in the bolt or channel area is unique for the selected bolt or channel and the layout for the data in the bolt or channel area depends on the data layout chosen.

In this Section

- Common Area Overview
- Bolt or Channel Area Overview