# Manual Mode - 10061

Used to set the Virtual Station in manual mode.

If the signal is True (high) the signal 101 - Manual mode is high.
If the signal is False (low) the signal 101 - Manual mode is low.

Name in SoftPLC: SET_MANUAL_MODE

Converter | Signal Type | Value Type | Size Min [bit] | Size Max [bit]
--- | --- | --- | --- | ---
Standard | State | Boolean | 1 | 1
Invert | State | Boolean | 1 | 1

To avoid duplicating signals, it is possible to define Value Converters.

Converters are used to support more than one representation of the same signal (for example Angle/Torque Status can both be represented bitwise or as a status character).

Relevant Information

- Manual Mode - 101

## Devices

- Fieldbus: TRUE

- Indicator Box: FALSE

- Internal I/O: TRUE

- Operator Panel: TRUE

- Tool Functions: FALSE

- ST Selector: FALSE

- Stacklight: TRUE

- TLS Tag: FALSE

- I/O Expander: TRUE