# Adding Acyclic Result Configuration in the Bolt or Channel Area

1. Select Add in the bolt or channel area.

   The Create acyclic result configuration window opens.

2. Select a parameter from the Multistep tightening, Program monitor, Program restriction, Step monitor or Step restriction drop-down menu .

3. Select the Output Data Type, enter the offset value, identifier and enter the size if the Output Data Type selected was a string.

   For Step monitor and Step restriction, select the step category and choose between Soft start, Rundown, Start and Final.

   Instead of the step number, indicate which step category results should be displayed.

   If there are several steps with the same step category, you can choose to show the step that is Last executed or Last in program (the step with higher order number) in the Step category chooser drop-down menu.

4. Select Add and then Close.