# SoftPLC Configurator Installation

To be able to use the SoftPLC functionality in a controller, the SoftPLC Configurator must be installed on the computer where a ToolsTalk 2 Client is installed.

1. Insert a USB device or similar, containing the MultiProg551_Atlas_Installation.

2. Double-click on Installation.bat in MultiProg551_Atlas_Installation, the installation starts.

3. Open the ToolsTalk client when the installation is completed (no restart required).

4. In the ToolsTalk 2 client, go to the Fieldbus and SoftPLC tab. Select the SoftPLC configuration section and in the General SoftPLC Settings, set SoftPLC to On.

Relevant Information

- Pushing Configurations to a Controller