# Input and Output Combination

Certain components, like a push-button, may be mapped with both an Output Signal (lamp) and an Input Signal (button). The output signal is valid during a programmable duration or until the next tightening starts. The input signal is continuously sampled by the controller.

All the different accessories show where and how an output signal can be mapped.

## Mapping an output signal to a position:

1. Select a component or a position.

2. Select a component type from the drop-down menu. The following selections and parameter entry boxes, depend on the selected component type.

3. Select an Output Signal from the drop-down menu.

4. Set the Duration switch to Time or to Next tightening.

5. If Time is selected, a parameter entry box appears. Enter the duration of the output signal in seconds.

6. Set the Pulsating position switch to On for a flashing or intermittent signal, or to Off for a steady signal.

7. Select an Input Signal from the drop-down menu.