# Tool Configuration - Function Button

Use the tool's Function Button to control up to six of the available input signals. The buttons have three possible condition states that are combined with the two possible states of the direction switch.

Function button states | Direction switch states
--- | ---
Pressed | CW
Single push | CW
Double push | CW
Pressed | CCW
Single push | CCW
Double push | CCW

Two configurable parameters controls the push time.

Parameter | Description | Default value
--- | --- | ---
Push detection interval (ms) | For single push: the maximum push time (in milliseconds) between the button being pressed and the button being released. | 300 ms
Next push interval (ms) | For double push: the maximum time (in milliseconds) between the button being released after the first push, and the button being pressed again. | 300 ms