# Input Signal Configuration

An input signal can be mapped to a button, switch or a terminal connector. The signals are continuously sampled by the controller.

Event input signals trigger the controller. One example is to press a push button and then release it.

State input signals are active as long as the signal is present. One example is a key switch. Another example is to press a push button and keep it pressed.

All the different accessories show where and how an input signal can be mapped.

## Mapping an input signal to a position:

1. Select a component or a position.

2. Select a Signal from the drop-down menu.

Certain components, for example two-way switches, may be configured with two input signals.