# Running a Forced by Piece Route

1. Attach the required tool to the controller.

2. Send the required route(s) with Forced by piece sequence to the STRwrench controller.
   For further information, refer to Adding a Route via QA Supervisor.

3. On the EHMI home menu, tap Route.

4. On the Route page, tap the route name or tap Run .

5. In the Inspections category of the Edit Route page, on the row of the inspection to run, tap Run .

In case of tests configured with traceability tags, the tags are requested during the test through dialogs that are displayed on the EHMI according to the tags' configuration.
If a traceability tag is configured as optional, it is possible to skip the tag request by tapping Skip tag .
Fore more information, refer to Traceability Tags.

If the route has been configured with the Skip option enabled and the tag's Collection Point is set to Before, it is also possible to skip the whole measurement by tapping Skip measurement / inspection . Note that if a measurement of a forced by piece route is skipped, it is not possible to run it later.

In this Section

- Navigating a Forced by Piece Route