# Measure angle from

Below an example of a complete curve in which the measurement of the angle starts as soon as the torque reading starts, to be compared with the curves representing the angle measured from One step/Second step/Starting second step:

A | Torque [Nm] | B | Angle [°]
C | Time [ms] |  |

One step: the measurement of the angle starts as soon as the Final monitoring torque value is reached.

A | Torque [Nm] | B | Angle [°]
C | Time [ms] |  |

Second step: the measurement of the angle starts in the second step, when the Final angle monitoring torque value is reached.

A | Torque [Nm] | B | Angle [°]
C | Time [ms] |  |

Starting second step: the measurement of the angle starts at the starting of the second step.

A | Torque [Nm] | B | Angle [°]
C | Time [ms] |  |

## Applies to: