# Summary category for Cm/Cmk and CAM/Cpk CNOMO

On the upper part of the Run inspection page, tap Summary to displayed the statistics parameters related to the measured torque/angle values.

The following parameters are shown:

- Test results: result of the test (OK, NOK).

- Minimum Cm (Minimum CAM): value of minimum Cm (CAM), configured in the inspection.

- Cm (CAM): value of the Cm (CAM) index calculated, by using the measured values.

- Minimum Cmk (Minimum Cpk): value of minimum Cmk (Cpk), configure in the inspection.

- Cmk (Cpk): value of the Cmk (Cpk) index, calculated by using the measured values.

- Lower average limit: value of Lower average control limit, configure in the inspection.

- Upper average limit: value of Upper average control limit, configure in the inspection.

- Torque average: value of Torque average, calculated by using the measured values.

To restart the test: on the upper-right corner of the Summary category, tap Restart test.

To exit the test: on the upper-right corner of the Summary category, tap End test.

If the batch is completed, after the End test is tapped, the test is closed without showing any Confirmation message.

If the batch is not completed or the batch is set to zero, after the End test is tapped, a Confirmation massage is displayed.

To print the test report: on the upper-right corner of the Summary category, tap Print report.

To print the test label: on the upper-right corner of the Summary category of the Cm/Cmk inspection, tap Print label.

In the label, the following information are shown:

- Barcode related to the Tool ID.

- Tool ID

- Nominal value of the test (torque, angle or both)

- Location of the tool

- Test date

- Date of the next test

- Cm/Cmk values. The values are negative if the test is NOK

## Applies to: