# Measuring Devices

The measuring devices section describes how to connect the device to the related measuring device (IRC-Connect, STwrench, STRwrench, STbench - in case of STpad, STpad cable adapter - in case of STpad).

The IRC-Connect and the STwrench need the bluetooth connection to be used.

The device can store up to 100 measuring devices into its own memory.
Start STpad to display the Home page. Then select Measuring Devices between the available features.
The following is displayed:

A | Command buttons | B | List of measuring devices

Below are the columns that define the list of Measuring devices:

- Name: it is the name of the measuring device paired/connected to the device.

- Serial number: it is the serial number of the measuring device paired/connected to the device.

- Device type: it is the type of the measuring device paired/connected to the device.

- Connection type: it is the connection type of the measuring device paired/connected to the device.
  The connections types are:

  - IRC-B: for IRC-Connect, STwrench and STRwrench.

  - TCP/IP: for STbench and STRwrench.

  - USB: for STpad cable adapter.

- Status: it is the status of the measuring device paired/connected to the device. The available status are:

  - not paired: the measuring device has been created but it has never been paired with STpad.

  - paired: the configured measuring device has been paired with STpad.

  - connection up: the measuring device is connected with STpad.

  - connection down: the measuring device is off or out of range.

When a measuring device is disconnected from STpad, its status is Paired

For each measuring device type, only one Measuring device per time can be connected to the device.

It is possible to sort the columns that define the list of Measuring devices either in ascending or descending alphabetical order, according to customer needs. Hence, tap the column to be sorted (in the screen above the column NAME is selected): the up arrow (placed on the right of the column heading) lists the Measuring devices Name (or Serial Number / Device Type / Connection Type / Status) details in ascending alphabetical order; on the other hand, the down arrow lists the Measuring devices Name (or Serial Number / Device Type / Connection Type / Status) details in descending alphabetical order.

It is possible to customize the sequence of the columns that defines the list of Measuring devices, according to the customer needs. Hence, tap the column heading to be moved (i.e. NAME, SERIAL NUMBER, DEVICE TYPE, CONNECTION TYPE or STATUS); finally drag and drop it on the necessary position.

Relevant Information

- Deleting a Measuring Device
- Pairing the IRC-Connect

In this Section

- Deleting a Measuring Device
- Searching a Measuring device
- IRC-Connect
- STwrench
- STbench
- STpad cable adapter
- STRwrench

## Applies to: