# Running a forced by piece Route

1. Connect the device to the necessary measuring device (for more information, see “Measuring devices”).

2. Import the necessary route(s) with "Forced by piece" sequence on the device (for more information, see “Adding Route(s) through the Template file”).

3. In the Route page, tap Play in correspondence of the enabled inspection.

In this Section

- Navigating a forced by piece Route

## Applies to: