# Adding a Visual inspection

1. In the Home page, tap Parts.

2. In the Parts page, tap a configured part.

3. On the upper part of the Edit part page, tap Inspections.

4. On the upper-right part of the Inspection category, tap Add.

5. In the Test type window, tap one of the Visual check inspections. In the following, an example of the Visual check- attribute inspection page. The structure is the same for all the inspections, only the categories change.

   A | Categories | B | Save button
   C | Parameters |  |

6. In the General category of the Add visual – inspection page, configure the inspection parameters.

7. In the Add visual – inspection page, tap Picture.

8. In the Picture category, it is possible to:

   - Add an image/video: on a USB storage device, save the image/video to use in a folder named media_items, connect the storage device to the STpad and tap the Add button on the right side of the Picture page. In the Add picture dialog box, select the image/video to load and click OK.

     The maximum size of images is 5 MB, the maximum size of videos is 10 MB.

   - Remove a picture: on the right side of the Picture page, tap the Remove button.

9. In the Add visual – inspection page, tap Traceability.

10. In the Traceability category of the Add visual – inspection page, configure the following parameters:

    - Verification code: type the verification code that must be entered or scanned when the inspection is run. This field is case-sensitive.

    - Verification code description: to guide the operator, type the description of the verification code dialog box that is displayed when the inspection is run.

    Assignable causes: it is possible to:

    - List:

      - select an assignable causes list: tap the Search icon () and then select an already configured item in the Assignable causes list page.

      - add a new assignable causes list: tap the Search icon (); on the upper-right corner of the Assignable causes list page, tap Add to configure a new item.

      - delete the link to the assignable causes list: tap the Delete icon ().

    - Mandatory: if the check box is selected, the operator must select/type an assignable cause to continue the test.

    - Force selection from list: select between:

      - No: the operator can type the assignable cause, without selecting it from the list.

      - Yes: the operator can only select the assignable cause from the list.

      - Inherit: the selection from list can be forced or not forced, depending on the definition of this parameter in the Assignable causes list page.

    Corrective actions: it is possible to:

    - List:

      - select a corrective actions list: tap the Search icon () and then select an already configured item in the Corrective actions list page.

      - add a new corrective actions list: tap the Search icon (); on the upper-right corner of the Corrective actions list page, tap Add to configure a new item.

      - delete the link to the corrective actions list: tap the Delete icon ().

    - Mandatory: if the check box is selected, the operator must select/type a corrective action to continue the test.

    - Force selection from list: select between:

      - No: the operator can type the corrective action, without selecting it from the list.

      - Yes: the operator can only select the corrective action from the list.

      - Inherit: the selection from list can be forced or not forced, depending on the definition of this parameter in the Corrective actions list page.

11. On the upper-right corner of the Add visual – inspection page, tap Save.

## Applies to: