# Results category

In the Results category of the Run inspection page, the following items are shown:

- On the left side of the Results category, the variable chart shows a plot with all the results of the inspection.
  By selecting a result from the variable chart, the relative value is highlighted in the result table on the right, and vice versa.

- On the right side of the Results category, the batch size counter () indicates the number of the results to do.
  If the batch size is set to zero, only the progressive index of the results is displayed ().
  If the batch size is greater than zero, the batch is displayed as "number of results done/total number of results to do" ().

- On the right side of the Result category, the Tuning brake button optimizes the braking. By selecting the Tuning brake button, the test is restarted.

- On the right side of the Results category, the following command buttons are displayed:

  - To delete the whole set of results (when enabled by external software), tap the following icon: .
    For SPC (tool) inspection, it is not possible to delete a result if the subgroup is completed.
    For tests run on motorized cells: in the event the test is stopped by opening the safety cage, when the cage is closed again it is possible to delete all the results and automatically restart the test.

  - To delete one result (when enabled by external software), select it and tap the following icon: .

  - To add a comment to a result, select it and tap the following icon: .

  - To add a picture to a result, select it and tap the following icon: .

- On the right side of the Results category, the results table shows all the values acquired during the test.

  If a result is NOK, the related value in the results table is highlighted with a red colored bar.

- On the lower-right corner of the Result category, the brake status indicator shows that the measuring device is ready for the test (blue indicator ), or that the measuring device is not ready for the test (red indicator ).
  If the indicator is red, wait until the indicator turns blue before acquiring the next value.

- In the lower part of the Result category, the following summary of the values acquired are shown:

  - Minimum: minimum value among the results of the inspection.

  - Maximum: maximum value among the results of the inspection.

  - STD (σ): Standard deviation (indicated with the Greek letter “Sigma”) of the results of the inspection. At the beginning the STD (σ) value is equal to 0 and changes after at least two results.

  - Average: average value of the results of the inspection.

  - Cm and Cmk values change after reaching the number of samples defined during the inspection definition. If the number of samples is equal to 0, Cm and Cmk values change after three results.

- To stop a test running on a motorized cell, in the bottom-right corner of the Results category click the Stop button. If you then delete all the collected results by tapping , the test restarts automatically.
  The Stop button is available only for tests run on motorized cells.

## Applies to: