# Adding a multistep inspection

Multistep strategy is used when the tool performs multiple operations during the same tightening and those steps need to be evaluated.

1. In the Tool page, tap a configured power tool.

   The Cm/Cmk multistep inspection is available only for Power tool

2. On the upper part of the Edit tool page, tap Inspection.

3. On the upper-right corner of the Inspection category, tap Add.

4. In the Test type window, select Cm/Cmk ISO. The following is displayed:

   A | Categories | B | Save button
   C | Parameters |  |

5. In the General category of the Add Cm/Cmk inspection page, configure the displayed parameters

6. On the upper part of the Add Cm/Cmk inspection page, tap Steps.

7. On the upper-right corner of the Step 1 section of the Steps category, tap the Edit icon() to set the parameters related to a specific step.

   The following is displayed:

8. In the Edit first step dialog box, configure the step parameters.

9. On the lower-right corner of the Edit first step dialog box, tap OK.

   To add a new step, tap the Add step icon ()

   The maximum number of steps allowed for each Inspection is equal to 30.

   After the step is configured, in the Step section, the following information are shown:

   - Step type: maximum value of the variable under test (torque/angle).

   - Simulation torque: minimum value of the variable under test (torque/angle).

   - Simulation angle: minimum value of the variable under test (torque/angle).

   - Check type: minimum value of the variable under test (torque/angle).

   - Torque/Angle limits: minimum value of the variable under test (torque/angle).

   - Used for result: if the Used for result check box has been selected the icon is displayed.

10. On the upper part of the Add Cm/Cmk inspection, tap Picture. In this page the picture sent by external software is shown.

11. In the Picture category, it is possible to:

    - Add an image/video: on a USB storage device, save the image/video to use in a folder named media_items, connect the storage device to the STpad and tap the Add button on the right side of the Picture page. In the Add picture dialog box, select the image/video to load and click OK.
      The maximum size of images is 5 MB, the maximum size of videos is 10 MB.

    - Remove a picture: on the right side of the Picture page, tap the Remove button.

12. On the upper part of the Add inspection, tap Traceability.

13. In the Traceability category of the Add inspection page, configure the following parameters:

    - Verification code: type the verification code that must be entered or scanned when the inspection is run. This field is case-sensitive.

    - Verification code description: to guide the operator, type the description of the verification code dialog box that is displayed when the inspection is run.

    Assignable causes: it is possible to:

    - List:

      - select an assignable causes list: tap the Search icon () and then select an already configured item in the Assignable causes list page.

      - add a new assignable causes list: tap the Search icon (); on the upper-right corner of the Assignable causes list page, tap Add to configure a new item.

      - delete the link to the assignable causes list: tap the Delete icon ().

    - Mandatory: if the check box is selected, the operator must select/type an assignable cause to continue the test.

    - Force selection from list: select between:

      - No: the operator can type the assignable cause, without selecting it from the list.

      - Yes: the operator can only select the assignable cause from the list.

      - Inherit: the selection from list can be forced or not forced, depending on the definition of this parameter in the Assignable causes list page.

    Corrective actions: it is possible to:

    - List:

      - select a corrective actions list: tap the Search icon () and then select an already configured item in the Corrective actions list page.

      - add a new corrective actions list: tap the Search icon (); on the upper-right corner of the Corrective actions list page, tap Add to configure a new item.

      - delete the link to the corrective actions list: tap the Delete icon ().

    - Mandatory: if the check box is selected, the operator must select/type a corrective action to continue the test.

    - Force selection from list: select between:

      - No: the operator can type the corrective action, without selecting it from the list.

      - Yes: the operator can only select the corrective action from the list.

      - Inherit: the selection from list can be forced or not forced, depending on the definition of this parameter in the Corrective actions list page.

14. In the Add Cm/Cmk inspection page, tap Save.

To delete a step:

You can use this function only in intermediate steps. You cannot delete the first or last step.

1. In the Step category of the Add Cm/Cmk inspection page, select the step to delete.

2. In the Step section, tap the Delete icon () to delete the step.

To change the order of the steps:

1. In the Step category of the Add Cm/Cmk inspection page, select the step to move.

2. On the lower pat of the Step section, tap the backward/forward arrow to change the order of the steps.

## Applies to: