# Quick Programming - General Information

Quick Programming is a function that starts a test in a short time as specified in Quick Programming Default Values paragraph.
Before starting the quick programming test, connect the device to the related measuring device (for more information, see “Measuring devices”).
In case the device is connected to the STbench, run the Quick programming test through one of the following transducers: Brake, IRTT, IRTT T/A, SRTT, MT TS, Motorized cell.
In case the device is connected to the IRC-Connect or Cable Adapter, run the Quick programming test through one of the following transducers: IRTT, IRTT T/A, SRTT, MT TS.

Transducers and brake/cell operating working range: from 10% to 100% of the capacity.

The device automatically creates a default inspection (associated to a default tool) according to the tool, the connected transducer and the selected tool strategy.

For IRTT, IRTT T/A, SRTT, the following tool strategies are available: Click wrench – Click wrench, Click wrench - Cam-over, Peak – Peak, Power tool – Direct driven, Pulse tool – Pulse tool, Pulse tool – ACTA Pulse tool, Power tool - Only angle.
For MT TS, the following tool strategies are available: Click wrench – Click wrench, Click wrench - Cam-over, Peak – Peak, Power tool – Direct driven.
For brakes, the following tool strategies are available: Click wrench – Click wrench, Click wrench - Cam-over, Peak – Peak, Power tool – Direct driven, Power tool - Only angle.
For Motorized Cell, the following tool strategies are available: Click wrench – Click wrench, Click wrench - Cam-over, Peak – Peak.

For Motorized Cell it appears a window "Choose the parameters" with a selection of:

- Tightening Direction: Clockwise/Counterclockwise

- Target Torque: from 20% to 100% of Motorized Cell Nominal Torque

- Number of samples: (0-1000)

For details refer to Tool Inspection paragraph.

It is possible to change the default inspection / tool that define the Quick programming test, according to customer needs. Moreover, users can also save the default inspection / tool in the related sections.

Relevant Information

- Measuring Devices

In this Section

- Running a quick programming

## Applies to: