# Isolated mode

The Isolated mode is a internal service test to check brake(s) calibration on the STbench or calibrates a transducer with the STPad cable adapter.

In Isolated mode, the device does not store the results in the memory and does not generate any statistics. In order to perform this test properly, the calibration equipment is necessary.

In the Home page, select Isolated mode between the available features.

The following is displayed:

In this Section

- Doing a test

## Applies to: