# JJF 1610:2017 parameters

The JJF 1610:2017 inspection is available only for Power tools.

General category

- Name: type the name of the inspection.

- Barcode identifier (*): it identifies the inspection. If left blank, the identifier corresponds to the inspection name.

- Measuring device type: select the measuring device which runs the test. Below are the available options:

  - Manual selection

  - STpad cable adapter

  - STbench

  - IRC-Connect

- Measuring device S/N: type the serial number of the measuring device connected to the device.

- Number of samples: type the number of results to do during the test. This parameter ranges from 5 to 99. By default, the number of samples is set to 10.

- Tightening direction: from the drop down list, select the tightening direction. The available items are Clockwise and Counterclockwise.

- Free rounds: type the number of free rounds the tool performs to reach the proper operating speed before starting the test operation. By default, the number of free rounds is set to 3.

- Filter frequency: type the value of the filter frequency. This parameter ranges from 100 Hz to 2000 Hz. By default, the filter frequency is set to 500 Hz.

- Preload: select the checkbox to enable the preload measurements.

Calibration point 1 category

- Target torque: this parameter is defined in the JJF 1610:2017 standard. The default value of the target torque is equal to the tool minimum capacity.

- Measure angle from: from the drop-down list, select between:

  - One step: the measurement of the angle starts as soon as the Final monitoring torque value is reached.

  - Second step: the measurement of the angle starts in the second step, when the Final angle monitoring torque value is reached.

  - Starting second step: the measurement of the angle starts at the starting of the second step.

- Final angle monitoring: the default value of the final angle monitoring is half of the target torque.

- Hard joint angle: the default value of the hard joint angle is equal to 15.0 °.

- Soft joint angle: the value of the soft joint angle is equal to 360.0 °.

- Transducer S/N: type the serial number of the transducer linked to the measuring device connected to the device.

Calibration point 2 category and Calibration point 3 category have the same structure of Calibration point 1, only the target torque changes.

In Calibration point 2 category, the target torque is set to the 60% of the tool maximum capacity.

In Calibration point 3 category, the target torque is set to the 100% of the tool maximum capacity.

To run only the Calibration point 1 phase of the inspection, tap on the Calibration point 3 category and unselect the Enabled check box. Then, tap on the Calibration point 2 category and unselect the Enabled checkbox.

## Applies to: