# Connecting the device to the STwrench

1. Pair the STwrench to be connected to the device (for more information, see the paragraph Pairing STwrench).

2. In the Home page, tap Measuring Devices.

3. In the Measuring devices page, tap the STwrench to be connected to the device.

4. On the upper-right corner of the Edit STwrench page, tap Connect.

   If the connection process succeeds, on the upper-right corner of the device screen the STw icon is shown and on the STwrench display the IRCW icon is shown

In the Measuring device table, the Status of the STwrench is Connection up.

To open the Measuring device page, tap the left arrow near Edit STwrench.

If the STwrench is added on the device memory but it is not paired, in the Measuring Devices page, the Status of the STwrench is Not paired.

If the STwrench is paired to the device but not connected, in the Measuring Devices page, the Status of the STwrenchis is Paired.

If the STwrench is connected to the device, but it is either off or out of range, in the Measuring Devices page, the Status of the STwrench is Connection down.

## Applies to: