# Configuring the Tool tracker

1. In the Home page, tap Configuration > External systems > Tool tracker

2. In the Tool tracker configuration page, configure the following parameters:

   - Enabled: select the check box to enable the recording of the information listed above.

   - Enable for SPC: select the check box to enable the recording of information for SPC inspections.

   - Enable for Cm/Cmk ISO: select the check box to enable the recording of information for Cm/Cmk ISO inspections.

   - File name: type the path of a file to record the result information. The file must be created by the operator.

   - Export mode: select between:

     - Measure by measure: the values of a measure are exported in the file after each completed measure.

     - Test completed: the measures are exported in the file when the test is completed or abandoned.

   - Exported file: select between:

     - Daily rotation: a new file is created when the first measure of the day is acquired.

     - Single test: a new file is created at the end of each test.

     - Unique: all the measures are exported in a single file.

3. In the upper-right corner of the Tool tracker configuration page, tap Save.

## Applies to: