# Part inspections

The available inspections type for the Parts are:

- Visual check – Attribute: this inspection is used when the user is asked to choose among a list of attributes that are visually inspected. It is possible to create a fixed list of attributes to be marked as OK or NOK for each specific inspection.

- Visual check – Binary: this inspection is used as go/no go test. This is the most suitable inspection when the result of a test is binary: passed or failed.

- Visual check – Instructions: this inspection is used when recommendations or separate instructions need to be shown to the measuring device user without requiring any specific action.

- Visual check – Picture: this inspection consists in taking a picture of the part to be inspected; it is possible to compare it with a reference picture uploaded from external software and confirm/reject the part in production.

- Dimensional check - Cp/Cpk

- Dimensional check - SPC

It is possible to save two inspections with the same name and the same target object.
A warning message is displayed to inform the operator that an inspection with the same name already exists.
Select Yes to save the inspection.
Select No not to discard the inspection.

In this Section

- Adding a Visual inspection
- Attribute inspection parameters
- Binary inspection parameters
- Instructions inspection parameters
- Picture inspection parameters
- Adding a Dimensional inspection
- Cp/Cpk dimensional parameters
- SPC dimensional parameters
- Deleting a Part inspection
- Editing Part inspection
- Running Part inspection

## Applies to: