# Connecting the device to the IRC-Connect

1. Pair the IRC-Connect to be connected to the device (for more information, see the paragraph Pairing the IRC-Connect).

2. In the Home page, tap Measuring Devices.

3. In the Measuring devices page, tap the IRC-Connect to be connected to the device.

4. On the upper-right corner of the Edit IRC-Connect page, tap Connect.

   If the connection process succeeded, on the upper-right corner of the device screen the IRC-C icon is shown.

   In the Measuring device table, the Status of the IRC-Connect is Connection up.

   To open the Measuring device page, tap the left arrow near Edit IRC-Connect.

If the IRC-Connect is saved on the device memory but it is not paired, in the Measuring Devices page, the Status of the IRC-Connect is Not paired.

If the IRC-Connect is paired to the device but not connected, in the Measuring Devices page, the Status of the IRC-Connect is Paired.

If the IRC-Connect is connected to the device, but it is either off or out of range, in the Measuring Devices page, the Status of the IRC-Connect is Connection down.

After each connection, in the General section of the Edit IRC-Connect page the firmware version of the IRC-Connect is updated.

Relevant Information

- Pairing the IRC-Connect

## Applies to: