# Adding Route(s) through the Template file

1. Generate the Template file for routes on a USB storage device (for more information, see Generating template for routes).

2. Put the USB storage device into the USB port of the own PC.

3. From the PC, open the USB storage device.

4. Open the file STpad_RouteImportFile.xlsm. The following is displayed:

   - Route Name: type the name of the route.

   - Type: select one of the available options: Tool, Joint, Part.

   - Tool ID / Joint name / Part name: type the Tool ID/name of the joint/name of the part in the same way as the ID/name specified for an existing tool/joint/part stored on the device (for more information, see “Tools/Joints/Part”). This box is case-sensitive.

   - Inspection Name: type the Inspection Name in the same way as the Inspection Name specified for an existing inspection. Pay attention: type only an inspection already linked to the tool/joint/part given in the previous Tool ID / Joint name / Part name box (for more information, see “Tools”). This box is case-sensitive.

   - Language: select the language from the related drop-down box.

   Check the Excel option for the workbook calculation. Open a Excel file and click File > Options. On left side of the Excel options dialog box, select Formulas > Automatic option for the Calculation options section.

5. Complete the file STpad_RouteImportFile.xlsm to define the necessary route(s).

   When all the fields are filled in, the Wrong field column becomes green.

6. Once the Wrong field column in correspondence of the new route(s) is green colored, click the blue button Sort and export to automatically generate the file STpad_RouteImportFile.stpad.

   The file STpad_RouteImportFile.stpad is automatically saved into the USB storage device.

   Only the file STpad_RouteImportFile.stpad can be correctly imported on the device (for more information, see Importing the route(s) on the device

7. Save and close the file STpad_RouteImportFile.xlsm.

8. Close and remove the USB storage device.

9. Connect the USB storage device to the device.

10. Import the route(s) saved in the file STpad_RouteImportFile.stpad on the device (for more information about how to import routes, see “Importing the route(s) on the device”).

11. Click the Menu icon > Route to check that the import of the route(s) is correctly done.

Relevant Information

- Generating the template file for routes
- Importing routes on the device
- Tools

## Applies to: