# Tool inspections

The Inspection category assigns the test type according to the tool previously specified.
The maximum number of Inspections per Tool is 60.
The device assigns the following inspections:

- Cm/Cmk ISO: it makes a Cm/Cmk test through the ISO statistics to evaluate the tool capability.

- SPC: it is a method of quality control in which statistical methods are used. It makes a series of tests to evaluate an average value to be compared with successive mean values on the X/R chart. By analyzing these points in sequence it is possible to monitor and control the process.

- ISO 5393: it makes a test with the selected tool in compliance with the ISO 5393 standards. For more information, see “ISO 5393 International Standard – Second Edition 1994-05-01”.

- ISO 6789:2003: it makes a test with the selected tool in compliance with the ISO 6789 standards. For more information, see “ISO 6789 International Standard – Third Edition 2003-04-01”.

- ISO 6789-2:2017 : it makes a test with the selected tool in compliance with the ISO 6789:2017 standards. For more information, see “ISO 6789-2:2017 International Standard ”.

- CAM/Cpk CNOMO: it makes a Cm/Cmk test through the CNOMO statistics to evaluate the tool capability. For more information, see “CNOMO International Standard (E41.32.110N) – Edition July 1990”.

- Calibration: it makes a calibration test to evaluate the tool capability. The calibration test calibrates power tools and pulse tools.

- VDI/VDE 2645-2: it makes a test with the selected tool in compliance with the VDI/VDE 2645-2 standards. For more information, see “VDI/VDE 2645-2 – September 2014”

- JJF 1610-2017: it makes a test with the selected tool in compliance with the JJF 1610-2017 standards. For more information, see “JJF 1610-2017 - 2017-05-28”.

Below is a list that links each tool type with the related available inspections:

- Click wrench: Cm/Cmk ISO, SPC, ISO 6789, ISO 6789-2:2017, and CAM/Cpk CNOMO.

- Power tool: Cm/Cmk ISO, SPC, ISO 5393, CAM/Cpk CNOMO, Calibration, VDI/VDE 2645-2 (only for motorized tools, continuously rotating), JJF 1610-2017.

- Peak: Cm/Cmk ISO, SPC, ISO 6789, ISO 6789-2:2017 and CAM/Cpk CNOMO.

- Pulse tool: Cm/Cmk ISO, SPC, CAM/Cpk CNOMO and Calibration.

It is possible to save two inspections with the same name and the same target objet. A warning message is displayed to inform the operator that an inspection with the same name already exists.
Select Yes to save the inspection.
Select No to cancel the inspection.

In this Section

- Adding a Tool inspection
- Cm/Cmk ISO parameters
- SPC parameters
- ISO 6789:2003 parameters
- ISO 6789-2:2017 parameters
- ISO 5393 parameters
- CAM/Cpk CNOMO parameters
- JJF 1610:2017 parameters
- Calibration parameters
- VDI/VDE 2465-2 - tool based parameters
- VDI/VDE 2465-2 - position based parameters
- Adding a multistep inspection
- Cm/Cmk multistep parameters
- CAM/Cpk CNOMO multistep parameters
- Adding a Tool check Inspection through the Template file
- Deleting Tool inspection
- Editing Tool inspection
- Running Tool inspection
- Calibrating Power Focus
- Calibrating PowerMACS
- Calibrating generic controllers

## Applies to: