# Pairing the IRC-Connect

1. In the Home page, tap Measuring devices.

2. On the upper-right corner of the Measuring devices page, tap Add

3. In the Measuring devices type window, tap IRC-Connect.

   After selecting IRC-Connect in the Measuring device type window, the Connection category is automatically displayed.

   The General category is automatically filled after the pairing process.

4. In the Connection category, configure the following parameters:

   - Connection type: not available. It is set to IRC-B.

   - Trace read: select one of the following option for the trace reading from the IRC-Connect:

     - Always: the traces are always read.

     - NOK only: only NOK traces are read.

     - Never: the traces are never read.

   - Gyro compensation: select the check box to enable the gyro compensation.

5. In the Connection category, tap on Pair.

6. Switch on the IRC-Connect pressing the Power button placed on the main panel:

   A | Main panel | B | Result LEDs
   C | Radio LED | D | Power button

7. After IRC-Connect boot sequence is completed, press the Power button for five times: after two seconds the Radio LED is lit steady, and the Result LEDs start blinking in sequence.

8. The IRC-Connect is now in pairing mode. Tap Pair on the STpad.

9. At the end of the pairing process, on the Pairing window tap OK .

   In the Add IRC-Connect page, the General section is automatically filled with the following information:

   - Name: name of the paired measuring device.

   - Serial number: serial number of the paired measuring device.

   - Firmware version: firmware version of the paired measuring device.

   - Notes: type the optional notes.

10. On the upper-right corner of the Add IRC-Connect page, tap Save.

## Applies to: