# Running a quick programming

1. In the Home page, tap Quick Programming.

2. In the Select transducer dialog box, select the transducer to use.

   If no devices are connected to the STpad, an error message is displayed.

3. In the Select tool strategy dialog box, select the strategy to use. The available strategies are:

   The tool strategy changes depending on the transducer selected.

   In case the selected transducer is IRTT, IRTT T/A, SRTT, the available tool strategies are the following (regardless of the measuring device connected): Click wrench – Click wrench, Power tool – Direct driven, Peak – Peak, Pulse tool – Pulse tool, Pulse tool - ACTA pulse tool.
   In case the selected transducer is an MT TS, the available tool strategies are the following (regardless of the measuring device connected): Click wrench – Click wrench, Click wrench - Cam-over, Peak – Peak, Power tool – Direct driven.

   In case the transducer selected is the brake, the tool strategies available are as follows (in this case the STbench is the measuring device connected): Click wrench – Click wrench, Power tool – Direct driven, Peak – Peak.

4. in the Quick programming page, tap Play () to run the inspection.

On the upper-right corner of the Quick programming page, tap Save to save the configuration of the Tool and the inspection configured by the quick programming.

The configuration of the Tool and Inspection is editable.

## Applies to: