# Reaction bar

In the Home page, tap Configuration > General settings > Reaction bar.

To configure the reaction bar warning, set the following parameters:

By enabling the warning, a popup is displayed each time a test is started.

- Warning enabled: select the check box to enable the warning messages.

  By default, the warning messages are enabled for power tools.

- Warning enabled for pulse tools: select the check box to enable the warning messages for pulse tools.

- Minimum suggested torque: type the minimum torque value from which a warning message suggesting the use of the reaction bar is displayed. The default value is 10 Nm.

  From the warning message, tap on OK to continue the test.

- Minimum mandatory torque: type the minimum torque value from which a warning message requiring the use of the reaction bar is displayed. The default value is 15 Nm.

  From the warning message, tap on OK to confirm that the reaction bar is use and start the test; if the reaction bar is not in use, tap on NO and cancel the test.

- Torque unit of measurement: from the drop-down list, select the unit of measurement.

## Applies to: