# Calibrating PowerMACS

1. Connect the system (for more information, see STbench Operation Manual / STpad Operation Manual – Operation – Calibrating PowerMACS - General Information).

2. Switch on both the device and the PowerMACS.

3. On the device, configure the PowerMACS (for more information, see Controllers).

4. After configuring the PowerMACS, configure the tool to calibrate (for more information, see Adding a Tool).

5. After configuring the tool to calibrate, configure the calibration inspection (for more information, see Adding a calibration inspection).

   At the end of the configuration of the calibration inspection, the following is displayed:

   A | Play

6. Tap Play for running the Inspection.

   If in the Controller category of the calibration inspection, Manual selection is selected, a synchronization mode dialog box appears during the calibration. Select the synchronization mode to continue the calibration process.

   At the end of the calibration inspection, the following is displayed:

   A | Calibration inspection Toolbar

   On the Calibration inspection Toolbar, the Results page shows a Torque chart with all the results of the inspection (on the right side), and the list of the results of the inspection (on the left side).

   Tap the Angle icon () placed on the upper right corner of the Torque chart to show the Angle chart:

7. On the Calibration inspection Toolbar, tap Summary to display the following page:

   Tap Save and Exit, to save the new scale factor on the tool calibrated.

   If a label printer is configured, a dialog box asking to confirm the printing of the label is displayed.

## Applies to: